SectionVerb {
	EnableSequence [
		cdev "hw:msm8974taikomtp"

		cset "name='SLIMBUS_0_RX Audio Mixer MultiMedia1' 1"
		cset "name='SLIM RX1 MUX' AIF1_PB"
	]

	DisableSequence [
		cdev "hw:msm8974taikomtp"

		cset "name='SLIMBUS_0_RX Audio Mixer MultiMedia1' 0"
	]

	Value {
		TQ "HiFi"

		PlaybackPCM "hw:msm8974taikomtp"
		CapturePCM "hw:msm8974taikomtp"
	}
}

SectionDevice."Speaker" {
	Comment "FP2 speaker"

	ConflictingDevice [
		"Headphones"
	]

	EnableSequence [
		cdev "hw:msm8974taikomtp"

		# We need to disable this while setting up the route, else the
		# driver will hang if the stream is open.
		cset "name='SLIMBUS_0_RX Audio Mixer MultiMedia1' 0"

		cset "name='SLIM_0_RX Channels' One"
		cset "name='RX7 MIX1 INP1' RX1"
		# default: 87
		cset "name='RX7 Digital Volume' 70"
		cset "name='SPK DRV Volume' 8"

		# Route has been set up, re-enable the mixer.
		cset "name='SLIMBUS_0_RX Audio Mixer MultiMedia1' 1"
	]

	DisableSequence [
		cdev "hw:msm8974taikomtp"

		# See comment in EnableSequence
		cset "name='SLIMBUS_0_RX Audio Mixer MultiMedia1' 0"

		cset "name='RX7 MIX1 INP1' ZERO"

		# Re-enabled in EnableSequence
	]

	Value {
		PlaybackChannels "1"
	}
}

SectionDevice."Headphones" {
	Comment "FP2 headphones"

	ConflictingDevice [
		"Speaker"
		"Earpiece"
	]

	EnableSequence [
		cdev "hw:msm8974taikomtp"

		# We need to disable this while setting up the route, else the
		# driver will hang if the stream is open.
		cset "name='SLIMBUS_0_RX Audio Mixer MultiMedia1' 0"

		cset "name='SLIM_0_RX Channels' Two"
		cset "name='SLIM RX2 MUX' AIF1_PB"
		cset "name='RX1 MIX1 INP1' RX2"
		cset "name='RX2 MIX1 INP1' RX1"
		cset "name='CLASS_H_DSM MUX' DSM_HPHL_RX1"
		cset "name='HPHL DAC Switch' 1"
		# default: 84
		cset "name='RX1 Digital Volume' 60"
		cset "name='RX2 Digital Volume' 60"

		# Route has been set up, re-enable the mixer.
		cset "name='SLIMBUS_0_RX Audio Mixer MultiMedia1' 1"
	]

	DisableSequence [
		cdev "hw:msm8974taikomtp"

		# See comment in EnableSequence
		cset "name='SLIMBUS_0_RX Audio Mixer MultiMedia1' 0"

		cset "name='SLIM_0_RX Channels' One"
		cset "name='SLIM RX2 MUX' ZERO"
		cset "name='RX1 MIX1 INP1' ZERO"
		cset "name='RX2 MIX1 INP1' ZERO"
		cset "name='CLASS_H_DSM MUX' ZERO"
		cset "name='HPHL DAC Switch' 0"

		# Re-enabled in EnableSequence
	]

	Value {
		PlaybackChannels "2"
	}
}

SectionDevice."Earpiece" {
	Comment "FP2 earpiece"

	ConflictingDevice [
		"Headphones"
	]

	EnableSequence [
		cdev "hw:msm8974taikomtp"

		# We need to disable this while setting up the route, else the
		# driver will hang if the stream is open.
		cset "name='SLIMBUS_0_RX Audio Mixer MultiMedia1' 0"

		cset "name='SLIM_0_RX Channels' One"
		cset "name='RX1 MIX1 INP1' RX1"
		# default: 84
		cset "name='RX1 Digital Volume' 60"
		cset "name='CLASS_H_DSM MUX' DSM_HPHL_RX1"
		cset "name='DAC1 Switch' 1"

		# Route has been set up, re-enable the mixer.
		cset "name='SLIMBUS_0_RX Audio Mixer MultiMedia1' 1"
	]

	DisableSequence [
		cdev "hw:msm8974taikomtp"

		# See comment in EnableSequence
		cset "name='SLIMBUS_0_RX Audio Mixer MultiMedia1' 0"

		cset "name='RX1 MIX1 INP1' ZERO"
		cset "name='CLASS_H_DSM MUX' ZERO"
		cset "name='DAC1 Switch' 0"

		# Re-enabled in EnableSequence
	]

	Value {
		PlaybackChannels "1"
	}
}
