From 238a72c97399dfb6d5b7fcb74acf619351f72bcd Mon Sep 17 00:00:00 2001
From: "Sicelo A. Mhlongo" <absicsz@gmail.com>
Date: Fri, 25 Feb 2022 22:46:23 +0200
Subject: [PATCH] ARM: dts: N900: use iio driver for accelerometer

---
 arch/arm/boot/dts/omap3-n900.dts | 53 +++++---------------------------
 1 file changed, 8 insertions(+), 45 deletions(-)

diff --git a/arch/arm/boot/dts/omap3-n900.dts b/arch/arm/boot/dts/omap3-n900.dts
index d40c3d2c4914..f53234ed9c0c 100644
--- a/arch/arm/boot/dts/omap3-n900.dts
+++ b/arch/arm/boot/dts/omap3-n900.dts
@@ -767,56 +767,19 @@ &i2c3 {
 
 	clock-frequency = <400000>;
 
-	lis302dl: lis3lv02d@1d {
-		compatible = "st,lis3lv02d";
+	lis302dl: lis302dl@1d {
+		compatible = "st,lis302dl";
 		reg = <0x1d>;
 
-		Vdd-supply = <&vaux1>;
-		Vdd_IO-supply = <&vio>;
+		vdd-supply = <&vaux1>;
+		vddio-supply = <&vio>;
 
 		interrupt-parent = <&gpio6>;
-		interrupts = <21 20>; /* 181 and 180 */
+		interrupts = <21 IRQ_TYPE_EDGE_RISING>, <20 IRQ_TYPE_EDGE_RISING>; /* 181 and 180 */
 
-		/* click flags */
-		st,click-single-x;
-		st,click-single-y;
-		st,click-single-z;
-
-		/* Limits are 0.5g * value */
-		st,click-threshold-x = <8>;
-		st,click-threshold-y = <8>;
-		st,click-threshold-z = <10>;
-
-		/* Click must be longer than time limit */
-		st,click-time-limit = <9>;
-
-		/* Kind of debounce filter */
-		st,click-latency = <50>;
-
-		/* Interrupt line 2 for click detection */
-		st,irq2-click;
-
-		st,wakeup-x-hi;
-		st,wakeup-y-hi;
-		st,wakeup-threshold = <(800/18)>; /* millig-value / 18 to get HW values */
-
-		st,wakeup2-z-hi;
-		st,wakeup2-threshold = <(900/18)>; /* millig-value / 18 to get HW values */
-
-		st,hipass1-disable;
-		st,hipass2-disable;
-
-		st,axis-x = <1>;    /* LIS3_DEV_X */
-		st,axis-y = <(-2)>; /* LIS3_INV_DEV_Y */
-		st,axis-z = <(-3)>; /* LIS3_INV_DEV_Z */
-
-		st,min-limit-x = <(-32)>;
-		st,min-limit-y = <3>;
-		st,min-limit-z = <3>;
-
-		st,max-limit-x = <(-3)>;
-		st,max-limit-y = <32>;
-		st,max-limit-z = <32>;
+		mount-matrix =	 "-1",  "0",  "0",
+				  "0",  "1",  "0",
+				  "0",  "0",  "1";
 	};
 
 	cam1: camera@3e {
-- 
2.35.1

