gpu_mem=64

# uncomment line to enable serial on ttyS0
# NOTE: This fixes the core_freq to 250Mh
#enable_uart=1

# to take advantage of your high speed sd card
dtparam=sd_overclock=100

# use drm backend ( for weston and wayland )
dtoverlay=vc4-fkms-v3d

# have a properly sized image
disable_overscan=1

# for sound over HDMI
hdmi_drive=2

# rotate the HDMI display
# 0 => no rotation
# 1 => 90 degrees clockwise
# 2 => 180 degrees clockwise
# 3 => 270 degrees clockwise
#display_hdmi_rotate=0

# Uncomment some or all of these to enable the optional hardware interfaces
#dtparam=i2c_arm=on
#dtparam=i2s=on
#dtparam=spi=on

# Enable audio (loads snd_bcm2835)
dtparam=audio=on

# custom CVT mode for HDMI
# see https://www.raspberrypi.org/documentation/configuration/config-txt/video.md
#hdmi_group=2
#hdmi_mode=87
#hdmi_cvt 800 480 60 6 0 0 0

# Automatically enable Bluetooth without having to use btattach
# Note that the Pi's Bluetooth interface is connected via hardware UART;
# if you intend to use it for other purposes (for example, serial debugging)
# comment out the line below.
dtparam=krnbt=on
