# Reference: <https://postmarketos.org/devicepkg>
pkgname=device-sharp-shl22
pkgdesc="SHARP SHL22"
pkgver=0.1
pkgrel=6
url="https://postmarketos.org"
license="MIT"
arch="armv7"
options="!check !archcheck"
depends="postmarketos-base linux-sharp-shl22 mkbootimg msm-fb-refresher"
makedepends="devicepkg-dev"
source="
	deviceinfo
	initfs-hook.sh
"

build() {
	devicepkg_build $startdir $pkgname
}

package() {
	devicepkg_package $startdir $pkgname

	# Disable v4l (video4linux), because without the camera firmware
	# blobs this makes dev hang with the kernel this device uses (#1033)
	mkdir -p "$pkgdir"/etc/udev/rules.d
	ln -s /dev/null "$pkgdir"/etc/udev/rules.d/60-persistent-v4l.rules
}


sha512sums="
f8e8a34307e02a2b56b7a7a4b4ec4d2f8afb563197a36cdd021edbf2549aec97db1e667cbe9275d9078742cbd4d6642ab01081c7c9f7fe79eaa5803d7166116a  deviceinfo
c983fc8281167bed1de5eec3651d82ed0dea612a4267acc8edf34ac8b1f857a57d5d63c555a373749eef3119cbfc9f4d25a080c0291d5af847642b5f60fcb211  initfs-hook.sh
"
