# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="OnePlus 5"
deviceinfo_manufacturer="OnePlus"
deviceinfo_codename="oneplus-cheeseburger"
deviceinfo_year="2017"
deviceinfo_arch="aarch64"

# Device related
deviceinfo_gpu_accelerated="true"
deviceinfo_chassis="handset"
deviceinfo_keyboard="false"
deviceinfo_external_storage="false"
deviceinfo_screen_width="1080"
deviceinfo_screen_height="1920"

# Bootloader related
deviceinfo_flash_method="fastboot"
deviceinfo_generate_bootimg="true"
deviceinfo_bootimg_qcdt="false"
deviceinfo_bootimg_dtb_second="false"
deviceinfo_flash_offset_base="0x00000000"
deviceinfo_flash_offset_kernel="0x00008000"
deviceinfo_flash_offset_ramdisk="0x01000000"
deviceinfo_flash_offset_second="0x00f00000"
deviceinfo_flash_offset_tags="0x00000100"
deviceinfo_flash_pagesize="4096"
deviceinfo_flash_sparse="true"

# Required for devices using UFS as storage (instead of e.g. eMMC)
deviceinfo_rootfs_image_sector_size="4096"

# Common mainline kernel options
deviceinfo_flash_kernel_on_update="true"
deviceinfo_dtb="qcom/msm8998-oneplus-cheeseburger"
deviceinfo_append_dtb="true"

# Close to mainline kernel options
# We need 'clk_ignore_unused' for now or we don't get graphics
deviceinfo_kernel_cmdline_mainline="clk_ignore_unused quiet loglevel=5 modprobe.blacklist=ipa"
deviceinfo_modules_initfs_mainline="panel-samsung-s6e3fa5 msm i2c-qup bq27xxx_battery_i2c rmi_i2c qcom_spmi_haptics"
deviceinfo_mesa_driver_mainline="msm"

# Alpine kernel options
deviceinfo_kernel_cmdline_alpine="PMOS_NO_OUTPUT_REDIRECT"
deviceinfo_modules_initfs_alpine="fixed qcom_glink_rpm qcom_smd-regulator qcom-apcs-ipc-mailbox gcc-msm8998 mmcc-msm8998 phy-qcom-qmp-ufs phy-qcom-qusb2 dwc3 dwc3-qcom nvmem_qfprom qcom-spmi-pmic qcom-pon governor_simpleondemand clk-smd-rpm ufs_qcom i2c-qup bam_dma rmi_i2c"
