# udev rules file
# All device names can be read from weston's logfile

# Touchscreen (use 'weston-calibrator' to calibrate)
SUBSYSTEM=="input", ATTRS{name}=="sec_touchscreen", \
ENV{ID_INPUT}="1", ENV{ID_INPUT_TOUCHSCREEN}="1"
