# Archived: Downstream port, only for testing. Use mainline port (oneplus-billie2)!
# Reference: <https://postmarketos.org/devicepkg>
pkgname=device-oneplus-billie2-downstream
pkgdesc="OnePlus Nord N100 (Downstream)"
pkgver=3
pkgrel=0
url="https://postmarketos.org"
license="MIT"
arch="aarch64"
options="!check !archcheck"
depends="postmarketos-base linux-oneplus-billie2 mkbootimg"
makedepends="devicepkg-dev"
source="deviceinfo kernel-cmdline.conf"

build() {
	devicepkg_build $startdir $pkgname
}

package() {
	devicepkg_package $startdir $pkgname
}

sha512sums="
63e427a6cb96589a4f8bddccf5ac22f27a59096c475160a695926cd91935dc67daf5ac2671b66f3b50f91d688e968c69acbaf390371348e0be700c9b25e59d8e  deviceinfo
4bc72fb80c18e99c656039f1bcfbdf7c4168e03a5ff5251de650b77e070d52797d68324d2b61f121e475a8370bb66bebf7db2dbf09fc5db75745a5e1f859d2de  kernel-cmdline.conf
"
