From 7fa37ba25a1dfc084e24ea9acc14bf1fad8af14c Mon Sep 17 00:00:00 2001
From: Arnd Bergmann <arnd@arndb.de>
Date: Thu, 7 Aug 2025 22:54:15 +0200
Subject: [PATCH] media: s5p-mfc: remove an unused/uninitialized variable

The s5p_mfc_cmd_args structure in the v6 driver is never used, not
initialized to anything other than zero, but as of clang-21 this
causes a warning:

drivers/media/platform/samsung/s5p-mfc/s5p_mfc_cmd_v6.c:45:7: error: variable 'h2r_args' is uninitialized when passed as a const pointer argument here [-Werror,-Wuninitialized-const-pointer]
   45 |                                         &h2r_args);
      |                                          ^~~~~~~~

Just remove this for simplicity. Since the function is also called
through a callback, this does require adding a trivial wrapper with
the correct prototype.

Fixes: f96f3cfa0bb8 ("[media] s5p-mfc: Update MFC v4l2 driver to support MFC6.x")
Cc: stable@vger.kernel.org
Signed-off-by: Arnd Bergmann <arnd@arndb.de>
Signed-off-by: Hans Verkuil <hverkuil+cisco@kernel.org>
---
 .../platform/samsung/s5p-mfc/s5p_mfc_cmd_v6.c | 35 +++++++------------
 1 file changed, 13 insertions(+), 22 deletions(-)

diff --git a/drivers/media/platform/samsung/s5p-mfc/s5p_mfc_cmd_v6.c b/drivers/media/platform/samsung/s5p-mfc/s5p_mfc_cmd_v6.c
index 47bc3014b5d8b8..f7c682fca64595 100644
--- a/drivers/media/platform/samsung/s5p-mfc/s5p_mfc_cmd_v6.c
+++ b/drivers/media/platform/samsung/s5p-mfc/s5p_mfc_cmd_v6.c
@@ -14,8 +14,7 @@
 #include "s5p_mfc_opr.h"
 #include "s5p_mfc_cmd_v6.h"
 
-static int s5p_mfc_cmd_host2risc_v6(struct s5p_mfc_dev *dev, int cmd,
-				    const struct s5p_mfc_cmd_args *args)
+static int s5p_mfc_cmd_host2risc_v6(struct s5p_mfc_dev *dev, int cmd)
 {
 	mfc_debug(2, "Issue the command: %d\n", cmd);
 
@@ -31,7 +30,6 @@ static int s5p_mfc_cmd_host2risc_v6(struct s5p_mfc_dev *dev, int cmd,
 
 static int s5p_mfc_sys_init_cmd_v6(struct s5p_mfc_dev *dev)
 {
-	struct s5p_mfc_cmd_args h2r_args;
 	const struct s5p_mfc_buf_size_v6 *buf_size = dev->variant->buf_size->priv;
 	int ret;
 
@@ -41,33 +39,23 @@ static int s5p_mfc_sys_init_cmd_v6(struct s5p_mfc_dev *dev)
 
 	mfc_write(dev, dev->ctx_buf.dma, S5P_FIMV_CONTEXT_MEM_ADDR_V6);
 	mfc_write(dev, buf_size->dev_ctx, S5P_FIMV_CONTEXT_MEM_SIZE_V6);
-	return s5p_mfc_cmd_host2risc_v6(dev, S5P_FIMV_H2R_CMD_SYS_INIT_V6,
-					&h2r_args);
+	return s5p_mfc_cmd_host2risc_v6(dev, S5P_FIMV_H2R_CMD_SYS_INIT_V6);
 }
 
 static int s5p_mfc_sleep_cmd_v6(struct s5p_mfc_dev *dev)
 {
-	struct s5p_mfc_cmd_args h2r_args;
-
-	memset(&h2r_args, 0, sizeof(struct s5p_mfc_cmd_args));
-	return s5p_mfc_cmd_host2risc_v6(dev, S5P_FIMV_H2R_CMD_SLEEP_V6,
-			&h2r_args);
+	return s5p_mfc_cmd_host2risc_v6(dev, S5P_FIMV_H2R_CMD_SLEEP_V6);
 }
 
 static int s5p_mfc_wakeup_cmd_v6(struct s5p_mfc_dev *dev)
 {
-	struct s5p_mfc_cmd_args h2r_args;
-
-	memset(&h2r_args, 0, sizeof(struct s5p_mfc_cmd_args));
-	return s5p_mfc_cmd_host2risc_v6(dev, S5P_FIMV_H2R_CMD_WAKEUP_V6,
-					&h2r_args);
+	return s5p_mfc_cmd_host2risc_v6(dev, S5P_FIMV_H2R_CMD_WAKEUP_V6);
 }
 
 /* Open a new instance and get its number */
 static int s5p_mfc_open_inst_cmd_v6(struct s5p_mfc_ctx *ctx)
 {
 	struct s5p_mfc_dev *dev = ctx->dev;
-	struct s5p_mfc_cmd_args h2r_args;
 	int codec_type;
 
 	mfc_debug(2, "Requested codec mode: %d\n", ctx->codec_mode);
@@ -129,23 +117,20 @@ static int s5p_mfc_open_inst_cmd_v6(struct s5p_mfc_ctx *ctx)
 	mfc_write(dev, ctx->ctx.size, S5P_FIMV_CONTEXT_MEM_SIZE_V6);
 	mfc_write(dev, 0, S5P_FIMV_D_CRC_CTRL_V6); /* no crc */
 
-	return s5p_mfc_cmd_host2risc_v6(dev, S5P_FIMV_H2R_CMD_OPEN_INSTANCE_V6,
-					&h2r_args);
+	return s5p_mfc_cmd_host2risc_v6(dev, S5P_FIMV_H2R_CMD_OPEN_INSTANCE_V6);
 }
 
 /* Close instance */
 static int s5p_mfc_close_inst_cmd_v6(struct s5p_mfc_ctx *ctx)
 {
 	struct s5p_mfc_dev *dev = ctx->dev;
-	struct s5p_mfc_cmd_args h2r_args;
 	int ret = 0;
 
 	dev->curr_ctx = ctx->num;
 	if (ctx->state != MFCINST_FREE) {
 		mfc_write(dev, ctx->inst_no, S5P_FIMV_INSTANCE_ID_V6);
 		ret = s5p_mfc_cmd_host2risc_v6(dev,
-					S5P_FIMV_H2R_CMD_CLOSE_INSTANCE_V6,
-					&h2r_args);
+					S5P_FIMV_H2R_CMD_CLOSE_INSTANCE_V6);
 	} else {
 		ret = -EINVAL;
 	}
@@ -153,9 +138,15 @@ static int s5p_mfc_close_inst_cmd_v6(struct s5p_mfc_ctx *ctx)
 	return ret;
 }
 
+static int s5p_mfc_cmd_host2risc_v6_args(struct s5p_mfc_dev *dev, int cmd,
+				    const struct s5p_mfc_cmd_args *ignored)
+{
+	return s5p_mfc_cmd_host2risc_v6(dev, cmd);
+}
+
 /* Initialize cmd function pointers for MFC v6 */
 static const struct s5p_mfc_hw_cmds s5p_mfc_cmds_v6 = {
-	.cmd_host2risc = s5p_mfc_cmd_host2risc_v6,
+	.cmd_host2risc = s5p_mfc_cmd_host2risc_v6_args,
 	.sys_init_cmd = s5p_mfc_sys_init_cmd_v6,
 	.sleep_cmd = s5p_mfc_sleep_cmd_v6,
 	.wakeup_cmd = s5p_mfc_wakeup_cmd_v6,
