maintainer="Antoine Martin (ayakael) <dev@ayakael.net>"
pkgname=device-pine64-pinenote
pkgdesc="Pine64 PineNote"
pkgver=9
pkgrel=0
_commit="28d2c05ab4e80a7972611cd3188f3e8be4197f6a"
url="https://postmarketos.org"
license="GPL-3.0-only"
arch="aarch64"
options="!check !archcheck"
# py3-numpy used by rockchip_ebc management libraries
depends="
	linux-pine64-pinenote
	postmarketos-base
	py3-numpy
	systemd-boot
	u-boot-pine64-pinenote
"
makedepends="devicepkg-dev sed python3"
# pinenote-dist repo provides some management scripts for pinenote and sway
# although for now we only source waveform scripts
source="
	pinenote-dist-$_commit.tar.gz::https://git.sr.ht/~hrdl/pinenote-dist/archive/$_commit.tar.gz
	waveform-extract-use-lib.patch
	sway-wayland-sessions-use-dbus.patch
	sway-waybar-config-fix-endless-interval-and-invisible-icons.patch
	sway-sane-scale.patch
	sway-nwg-menu-fix-css-path.patch

	deviceinfo
	kernel-cmdline.conf
	modules-initfs
	partition-table.txt

	pinenote-init-waveform.initd
	30-eink-waveform.files
	50-touchscreen.conf
	panfrost.conf
	tinydm-ebc-workaround-override.conf
"
subpackages="
	$pkgname-nonfree-firmware
	$pkgname-nonfree-firmware-openrc:firmware_openrc
	$pkgname-nonfree-firmware-systemd:firmware_systemd
	$pkgname-sway
	$pkgname-sway-hrdl
	$pkgname-systemd
	$pkgname-xournalpp
	$pkgname-x11
"
builddir="$srcdir"/pinenote-dist-$_commit

prepare() {
	default_prepare

	# use sh for scripts packaged in main pkg
	sed -i 's|#!/bin/bash|#!/bin/sh|' \
		bin/before_sleep.sh \
		bin/after_resume.sh
}

build() {
	devicepkg_build $startdir $pkgname
}

package() {
	devicepkg_package $startdir $pkgname

	install -Dm644 "$builddir"/etc/libinput/local-overrides.quirks \
		-t "$pkgdir"/etc/libinput

	# modprobe rules
	# cd because shellcheck-grep gets confused by usage of etc/modprobe.d
	(
		cd "$builddir"/etc

		install -Dm644 \
			./modprobe.d/rockchip_ebc.conf \
			./modprobe.d/wifi.conf \
			-t "$pkgdir"/usr/lib/modprobe.d

		# udev rules
		install -Dm644 \
			./udev/rules.d/81-libinput-pinenote.rules \
			./udev/rules.d/83-backlight.rules \
			./udev/rules.d/84-rockchip-ebc-power.rules \
			-t "$pkgdir"/usr/lib/udev/rules.d
	)

	# bins
	# rockchip_ebc_dump_buffers.py binary to dump whatever is on the screen framebuffer for debugging
	# {before,after}_sleep.sh hooks to put a splash screen when sleeping and shutdown backlight
	install -Dm755 \
		"$builddir"/bin/rockchip_ebc_dump_buffers.py \
		"$builddir"/bin/before_sleep.sh \
		"$builddir"/bin/after_resume.sh \
		-t "$pkgdir"/usr/bin

	# python library used by rockchip_ebc_dump_buffers and waveform extraction on first boot
	local _site_packages_path="$(python -c 'import site; print(site.getsitepackages())' | sed -e "s|\['||" -e "s|'\]||")"
	install -Dm755 "$builddir"/bin/rockchip_ebc_custom_ioctl.py \
		-t "$pkgdir"/$_site_packages_path

	# panfront sometimes insists on loading after rockchip_ebc
	install -Dm644 "$srcdir"/panfrost.conf \
		-t "$pkgdir"/usr/lib/modprobe.d

	# rockchip_ebc sometimes fails to load the initial waveform.
	# This forces a reload before starting tinydm
	# TODO: openrc workaround
	install -Dm644 \
		"$srcdir"/tinydm-ebc-workaround-override.conf \
		"$pkgdir"/usr/lib/systemd/system/tinydm.service.d/override.conf
}

hrdl() {
	pkgdesc="Opinionated sway UI by hrdl optimized for the Pinenote"
	install="$subpkgname.post-install $subpkgname.post-deinstall"
	depends="
		adwaita-icon-theme
		bash
		brightnessctl
		coreutils
		font-noto
		font-noto-emoji
		iio-sensor-proxy
		jq
		kitty
		lisgd
		network-manager-applet
		nwg-menu
		papirus-icon-theme
		postmarketos-ui-sway
		py3-dbus-next
		py3-i3ipc
		py3-pillow
		py3-pydbus
		rot8
		squeekboard
		swaybg
		swayidle
		thunar
		tinydm
		ttf-font-awesome
		waybar
		wtype
		wtype
		"

	# allows overwrite of menu-start.css
	replaces="nwg-menu"

	# greetd config
	install -Dm644  \
		"$builddir"/etc/greetd/environments \
		"$builddir"/etc/greetd/sway-config \
		-t "$subpkgdir"/etc/greetd

	# sway configs
	# nwg-menu hardcodes this location
	install -Dm644 \
		"$builddir"/etc/sway_hrdl/sway/colorscheme \
		"$builddir"/etc/sway_hrdl/sway/config \
		-t "$subpkgdir"/etc/sway_hrdl/sway
	install -Dm644 \
		"$builddir"/etc/sway_hrdl/waybar/config \
		"$builddir"/etc/sway_hrdl/waybar/style.css \
		-t "$subpkgdir"/etc/sway_hrdl/waybar
	install -Dm644 \
		"$builddir"/etc/sway_hrdl/nwg-panel/menu-start.css \
		-t "$subpkgdir"/usr/share/nwg-menu/

	# wayland session
	install -Dm644 \
		"$builddir"/wayland-sessions/sway_hrdl.desktop \
		-t "$subpkgdir"/usr/share/wayland-sessions

	# bins
	install -Dm755 \
		"$builddir"/bin/launch_lisgd.sh \
		"$builddir"/bin/toggle_menu.sh \
		"$builddir"/bin/sway_rotate.sh \
		"$builddir"/bin/sway_workspace \
		"$builddir"/bin/toggle_onscreen_keyboard.py \
		"$builddir"/bin/sway_dbus_integration.py \
		"$builddir"/bin/sway_hrdl \
		"$builddir"/bin/waybar_hrdl \
		-t "$subpkgdir"/usr/bin
}

xournalpp() {
	install_if="$pkgname=$pkgver-r$pkgrel xournalpp"
	depends="xournalpp"

	install -Dm644 \
		"$builddir"/config/xournalpp/settings.xml \
		"$builddir"/config/xournalpp/toolbar.ini \
		-t "$subpkgdir"/etc/skel/.config/xournalpp
}

firmware() {
	pkgdesc="WiFi, Bluetooth and display firmware"
	depends="linux-firmware-cypress linux-firmware-brcm"
	replaces="firmware-pine64-pinenote"

	# waveform firmware is provided locally via /dev/disk/by-label/waveform
	# extracted using waveform_exctract.sh, then adapted to kernel using wbf_to_custom.py
	# initd or systemd service execute these on first boot
	install -Dm644 "$srcdir"/30-eink-waveform.files \
		"$subpkgdir"/usr/share/mkinitfs/files/30-eink-waveform.files
	install -Dm755 \
		"$builddir"/bin/wbf_to_custom.py \
		"$builddir"/bin/read_file.py \
		"$builddir"/bin/waveform_extract.sh \
		-t "$subpkgdir"/usr/libexec/pinenote

	# create empty waveform firmware so that initial mkinitfs doesn't fail
	mkdir -p "$subpkgdir"/lib/firmware/rockchip
	touch "$subpkgdir"/lib/firmware/rockchip/ebc.wbf
	touch "$subpkgdir"/lib/firmware/rockchip/custom_wf.bin

	# symbolic link for wifi firmware to where drivers expects it
	mkdir -p "$subpkgdir"/lib/firmware/brcm
	ln -s ../cypress/cyfmac43455-sdio.bin.zst "$subpkgdir"/lib/firmware/brcm/brcmfmac43455-sdio.pine64,pinenote-v1.2.bin.zst
}

sway() {
	install_if="$pkgname=$pkgver-r$pkgrel sway"
	install="$subpkgname.post-upgrade"

	# dummy subpackage to allow seamless upgrade from 7-r0 to 8-r0,
	# which renamed `sway` to `sway-hrdl. Executes post-upgrade script
	# that changes default tinydm session back to vanilla sway, with
	# instructions to `apk add device-pine64-pinenote-sway-hrdl` to
	# use the opinionated non-default configuration
	# TODO: remove in preparation for v26.06 release
	mkdir -p "$subpkgdir"
}

systemd() {
	# post-install enables tinydm if tinydm-ebc was enabled
	# enables seamless upgrade 7-r0 to 8-r0
	# TODO: remove in preparation for v26.06
	install="$subpkgname.post-install"

	default_systemd
}

firmware_openrc() {
	install="$subpkgname.post-install"
	install -Dm755 "$srcdir"/pinenote-init-waveform.initd \
		"$subpkgdir"/etc/init.d/pinenote-init-waveform

	# source `install_if`, `pkgdesc` and `depends`
	default_openrc
}

firmware_systemd() {
	install -Dm644 \
		"$builddir"/systemd/pinenote-hrdl-extract-waveform.service \
		"$builddir"/systemd/pinenote-hrdl-convert-waveform.service \
		-t "$subpkgdir"/usr/lib/systemd/system

	# source `install_if`, `pkgdesc` and `depends`
	default_systemd
}

x11() {
	install_if="$pkgname=$pkgver-r$pkgrel xorg-server"

	# xorg touchscreen settings
	install -Dm644 "$srcdir"/50-touchscreen.conf \
		-t "$subpkgdir"/etc/X11/xorg.conf.d
}

sha512sums="
4b6548a05dcdbe1ddda97dba58d625407fb553f90817e8e678b97e28603f64aab9a31fa18bda654c06638f3be21d7a6936786197f93f715e7d03a07e380873c5  pinenote-dist-28d2c05ab4e80a7972611cd3188f3e8be4197f6a.tar.gz
780ece54589b4483461cc07917d9ca6f13222435872386d65c34ff6798758f28d81e913777d41b745e7bb0f53950b8f610ce361f2fe146937afd4080ae2aa904  waveform-extract-use-lib.patch
16f5c226d1366ebd0efc5bdc92a33ae184773a17ce593bdb71c60f1a091de13b2d39bedee43c46c01229e36d60f3688626a1b1ae08eab2c235ac6f5f0fc3d6a8  sway-wayland-sessions-use-dbus.patch
82babd0aa02084c7a05f7b2e3a6d74db373588cd612d4d75f5ec79db895d8bdda4fcde784a1b8340df33a8c5f26204151d55a9d9b9dd2cc317cef623f51b626e  sway-waybar-config-fix-endless-interval-and-invisible-icons.patch
4a02a3fb225b16290fbc469da5acba8438e959c0471743950ae125ede6b75b61e1772d900bd1f7c5fca55222cf430cae6c953d6065553ea3594babf33b569405  sway-sane-scale.patch
7effcd37bbf2cab66ccb57ab976de63c93bd03795ccd82f317fbfb16216da287ada4410d9b168057e651fa4d769588d1f0efa713caa28c5b71ba6b73909ae33c  sway-nwg-menu-fix-css-path.patch
ebe4ce7d3fc0a4dcb10cfeebd672b0d76e0f39ce34374629e42edad6173f0263043b483cbaa4cd4829e5a1441c28adbb448342ce6b42b839753ad6aa9ac32e80  deviceinfo
3a229912fad5d6aa8942fa987872cb0141c064f4bbbed813e9bcd0594ee4bdbf7c8715becb9e071c66ccd5f8b01cb8676686d8cdcf99b7a1f1abb1c9de38f7d4  kernel-cmdline.conf
e0d3ac808e7a4f05df327a824e30dc54864908e31f4a643f6e85f054ab812eeb28fef647eb52ae85bfad7d40c9cd81c43c1cdc575de5dbc04304d74862d9772c  modules-initfs
df0565391a66eed53ed817d3d1415bef000f9ed33ef2e8aa3016be3ecc21dd4a357e57838979d2710256776666dc01bfee8bf8a95b08a20a62d46cfbd8ac6c35  partition-table.txt
29710d80112f8797adf7e3dfd54771d8752d29cb265532e235fe406e380056ac846929568ddbe5110bbd74da337e2f8cd905e4092c14bc94aea07dc83f39aa6e  pinenote-init-waveform.initd
8f7a5ad2f407de8c474d54dfdb9cc099c96e8918fc123f8b2a8ff911d7e1c7ca6fe30f9cea8ee2f0c1ba5f3e53359193d0683ca912f0b66e79a12814ce38dd98  30-eink-waveform.files
ac433eebbc35a48561837495997aee4e55510b979bc0d8e3bafb761bc1be5b4bdeed2f456369dcbc582688aefd07c63966b0d72b6ffa99e84cfd868e677f02c8  50-touchscreen.conf
6ba6638754e00908243de2f73ed6898dac03638a200dcf7b7cd9684757355ee1eb0ac874af0f971ad2e054c1a8c471867bdaea4d9aaf7eea6d3cf81ac7dd73a2  panfrost.conf
3b95a2292a7367d228f281a1f0e031fffb3d26748350d7010d26b18a3fb46bceb214b083e0c8e2d5fe318c67ae3776663ad78fef83ce9030529d3a89b581b703  tinydm-ebc-workaround-override.conf
"
