# Archived: unmaintained port, only for testing. Use generic/mainline port (qcom-msm8953)
# Reference: <https://postmarketos.org/devicepkg>
pkgname=device-xiaomi-daisy
pkgdesc="Xiaomi Mi A2 Lite"
pkgver=15
pkgrel=0
url="https://postmarketos.org"
license="MIT"
arch="aarch64"
options="!check !archcheck"
depends="
	firmware-qcom-adreno-a530
	firmware-xiaomi-daisy
	linux-postmarketos-qcom-msm8953
	lk2nd-msm8953
	mkbootimg
	msm-firmware-loader
	postmarketos-base
	qbootctl
	soc-qcom-msm8953
	soc-qcom-msm8953-modem
"
makedepends="devicepkg-dev"
subpackages="$pkgname-fake-goodix:fake_goodix"

source="
	deviceinfo
	modules-initfs
	90-device-xiaomi-daisy.rules
"

build() {
	devicepkg_build $startdir $pkgname
}

package() {
	devicepkg_package $startdir $pkgname
}

fake_goodix() {
	pkgdesc="Calibration data for replacement goodix touch controllers"
	install -Dm644 90-device-xiaomi-daisy.rules -t "$subpkgdir/etc/udev/rules.d/"
}

sha512sums="
b9018241cf4aab7ca5399a39fb979b380bb91d12f888558754ae03edd4495367a5b9934c9562307b5d1bd380e4e3d5ccafd301a80a6b784ed87c44374ed4d0be  deviceinfo
7202f0a55dfe43348940412fc38e59c855594b070db8742419feadb2299086d5810107201a228b7137b7cc7a97c94afac95d81c0cd65c52f31dbcb619b0a4279  modules-initfs
a2608b01b7b6e2dade694af355ff4f0f26cad49cf54bc332c77eb75d19fdc985f7f996fedb72753de447be0391deabf5fcea52406791d1e6e0d165703b63f145  90-device-xiaomi-daisy.rules
"
