# Archived: unmaintained port, only for testing. Use generic/mainline port (qcom-msm8953)
pkgname=firmware-xiaomi-daisy
pkgver=2
pkgrel=2
pkgdesc="Firmware files for Xiaomi Mi A2 Lite"
url="https://postmarketos.org"
arch="aarch64"
license="proprietary"
_repository="firmware-xiaomi-daisy"
_commit="9ae200b57743088f83a6f2b02a6b7ce4596a77d6"
source="$pkgname-$_commit.tar.gz::https://github.com/alikates/firmware-xiaomi-daisy/archive/$_commit.tar.gz"
options="!strip !check !archcheck !spdx !tracedeps pmb:cross-native"
builddir="$srcdir/firmware-xiaomi-daisy-$_commit/gpu"

_fwdir="/lib/firmware/qcom/msm8953/xiaomi/daisy"

package() {
	# GPU firmwares
	install -Dm644 a506_zap.b02 -t "$pkgdir/$_fwdir"
	install -Dm644 a506_zap.mdt -t "$pkgdir/$_fwdir"
}

sha512sums="
0778b0c4a7e836c9e0cef842dda2fd9d5eba4693cd875a605413267690d48d9b7ea86b1ece0471e55e5c49d1b3645bee1aa735ba164d0120bdfc94ffffa7e16b  firmware-xiaomi-daisy-9ae200b57743088f83a6f2b02a6b7ce4596a77d6.tar.gz
"
