diff --git a/drivers/misc/mediatek/base/power/mt6735/mt_pbm.c b/drivers/misc/mediatek/base/power/mt6735/mt_pbm.c
index 138bde95..e4cc770b 100644
--- a/drivers/misc/mediatek/base/power/mt6735/mt_pbm.c
+++ b/drivers/misc/mediatek/base/power/mt6735/mt_pbm.c
@@ -20,8 +20,8 @@
 #include <mach/mt_pbm.h>
 #include <mach/upmu_sw.h>
 #include <mt-plat/upmu_common.h>
-#include <mt_cpufreq.h>
-#include <mt_gpufreq.h>
+#include "mt_cpufreq.h"
+#include "mt_gpufreq.h"
 #include <mach/mt_thermal.h>
 
 #ifndef DISABLE_PBM_FEATURE
diff --git a/drivers/misc/mediatek/base/power/mt6735/mt_pm_init.c b/drivers/misc/mediatek/base/power/mt6735/mt_pm_init.c
index b21d1b11..dd7b161f 100644
--- a/drivers/misc/mediatek/base/power/mt6735/mt_pm_init.c
+++ b/drivers/misc/mediatek/base/power/mt6735/mt_pm_init.c
@@ -30,7 +30,7 @@
 /* #include "mach/mt_cpufreq.h" */
 /* #include "mach/mt_gpufreq.h" */
 #include "mt_cpuidle.h"
-#include <mt_clkbuf_ctl.h>
+#include "mt_clkbuf_ctl.h"
 /* #include "mach/mt_clkbuf_ctl.h" */
 /* #include "mach/mt_chip.h" */
 #include "mt-plat/mtk_rtc.h"
diff --git a/drivers/misc/mediatek/base/power/mt6735/mt_ptp.c b/drivers/misc/mediatek/base/power/mt6735/mt_ptp.c
index fadec129..778d9328 100644
--- a/drivers/misc/mediatek/base/power/mt6735/mt_ptp.c
+++ b/drivers/misc/mediatek/base/power/mt6735/mt_ptp.c
@@ -145,7 +145,7 @@ unsigned int reg_dump_addr_off[] = {
 #include <linux/of_fdt.h>
 #endif
 /* local includes */
-#include <mt_spm.h>
+#include "mt_spm.h"
 #include "aee.h"
 #include <linux/gpio.h>
 
diff --git a/drivers/misc/mediatek/btcvsd/inc/mt6735/AudDrv_BTCVSD.h b/drivers/misc/mediatek/btcvsd/inc/mt6735/AudDrv_BTCVSD.h
index 2dbc586c..41d0eb7c 100644
--- a/drivers/misc/mediatek/btcvsd/inc/mt6735/AudDrv_BTCVSD.h
+++ b/drivers/misc/mediatek/btcvsd/inc/mt6735/AudDrv_BTCVSD.h
@@ -2,7 +2,7 @@
 #define AUDDRV_BTCVSD_H
 
 #include <linux/types.h>
-#include "AudioBTCVSDDef.h"
+#include "../../AudioBTCVSDDef.h"
 
 #undef DEBUG_AUDDRV
 #ifdef DEBUG_AUDDRV
diff --git a/drivers/misc/mediatek/cmdq/v2/cmdq_def.h b/drivers/misc/mediatek/cmdq/v2/cmdq_def.h
index 9c934827..b4a16437 100644
--- a/drivers/misc/mediatek/cmdq/v2/cmdq_def.h
+++ b/drivers/misc/mediatek/cmdq/v2/cmdq_def.h
@@ -9,7 +9,7 @@
 #ifdef CMDQ_COMMON_ENG_SUPPORT
 #include "cmdq_engine_common.h"
 #else
-#include "cmdq_engine.h"
+#include "mt6735/cmdq_engine.h"
 #endif
 
 #define CMDQ_SPECIAL_SUBSYS_ADDR (99)
diff --git a/drivers/misc/mediatek/ext_disp/extd_factory.c b/drivers/misc/mediatek/ext_disp/extd_factory.c
index a5ddf765..3e182033 100644
--- a/drivers/misc/mediatek/ext_disp/extd_factory.c
+++ b/drivers/misc/mediatek/ext_disp/extd_factory.c
@@ -4,7 +4,7 @@
 #include "extd_log.h"
 #include "extd_factory.h"
 #include "extd_info.h"
-#include "external_display.h"
+#include "mt6735/external_display.h"
 
 #include "dpi_dvt_test.h"
 
diff --git a/drivers/misc/mediatek/ext_disp/extd_multi_control.c b/drivers/misc/mediatek/ext_disp/extd_multi_control.c
index 5e88d3f8..8c796b58 100755
--- a/drivers/misc/mediatek/ext_disp/extd_multi_control.c
+++ b/drivers/misc/mediatek/ext_disp/extd_multi_control.c
@@ -3,8 +3,8 @@
 
 #include "extd_multi_control.h"
 #include "disp_drv_platform.h"
-#include "external_display.h"
-#include "extd_platform.h"
+#include "mt6735/external_display.h"
+#include "mt6735/extd_platform.h"
 #include "extd_log.h"
 #include "mtk_ovl.h"
 
diff --git a/drivers/misc/mediatek/fingerprint/gfx1xm/gfx1xm-spi.c b/drivers/misc/mediatek/fingerprint/gfx1xm/gfx1xm-spi.c
index cc9c58e4..a8a564d9 100644
--- a/drivers/misc/mediatek/fingerprint/gfx1xm/gfx1xm-spi.c
+++ b/drivers/misc/mediatek/fingerprint/gfx1xm/gfx1xm-spi.c
@@ -35,7 +35,7 @@
 #include <linux/proc_fs.h>
 #include <linux/completion.h>
 #include <mach/mt_clkmgr.h>
-#include <gfx1xm-spi.h>
+#include "gfx1xm-spi.h"
 #ifdef CONFIG_OF
 #include <linux/of.h>
 #include <linux/of_irq.h>
diff --git a/drivers/misc/mediatek/gpio/mt6735/6735_gpio.h b/drivers/misc/mediatek/gpio/mt6735/6735_gpio.h
index 4ed08308..5cb6be65 100644
--- a/drivers/misc/mediatek/gpio/mt6735/6735_gpio.h
+++ b/drivers/misc/mediatek/gpio/mt6735/6735_gpio.h
@@ -1,7 +1,7 @@
 #ifndef _6735_GPIO_H
 #define _6735_GPIO_H
 
-#include <mt_gpio_base.h>
+#include "mt_gpio_base.h"
 #include <linux/slab.h>
 #include <linux/device.h>
 
diff --git a/drivers/misc/mediatek/gpio/mt6735/mt_gpio_affix.c b/drivers/misc/mediatek/gpio/mt6735/mt_gpio_affix.c
index ce2d6c88..70d098a9 100644
--- a/drivers/misc/mediatek/gpio/mt6735/mt_gpio_affix.c
+++ b/drivers/misc/mediatek/gpio/mt6735/mt_gpio_affix.c
@@ -5,7 +5,7 @@
 #include <linux/device.h>
 /* #include <mach/mt_gpio.h> */
 #include <mt-plat/mt_gpio_core.h>
-#include <6735_gpio.h>
+#include "6735_gpio.h"
 
 
 void mt_gpio_pin_decrypt(unsigned long *cipher)
diff --git a/drivers/misc/mediatek/gpio/mt6735/mt_gpio_base.c b/drivers/misc/mediatek/gpio/mt6735/mt_gpio_base.c
index 1e35250f..e6e4b0e3 100644
--- a/drivers/misc/mediatek/gpio/mt6735/mt_gpio_base.c
+++ b/drivers/misc/mediatek/gpio/mt6735/mt_gpio_base.c
@@ -9,14 +9,14 @@
  ******************************************************************************/
 
 
-#include <6735_gpio.h>
+#include "6735_gpio.h"
 #include <linux/types.h>
 #include "mt-plat/sync_write.h"
 #include <mt-plat/mt_gpio.h>
 #include <mt-plat/mt_gpio_core.h>
-#include <mt_gpio_base.h>
+#include "mt_gpio_base.h"
 /* autogen */
-#include <gpio_cfg.h>
+#include "gpio_cfg.h"
 #ifdef CONFIG_OF
 #include <linux/of_address.h>
 #endif
diff --git a/drivers/misc/mediatek/gpio/mt6735/mt_gpio_base_linux.c b/drivers/misc/mediatek/gpio/mt6735/mt_gpio_base_linux.c
index 2cec43ad..8eb87094 100644
--- a/drivers/misc/mediatek/gpio/mt6735/mt_gpio_base_linux.c
+++ b/drivers/misc/mediatek/gpio/mt6735/mt_gpio_base_linux.c
@@ -6,7 +6,7 @@
 #include <linux/platform_device.h>
 #include <linux/seq_file.h>
 
-#include <mt_gpio_base.h>
+#include "mt_gpio_base.h"
 #include <mt-plat/mt_gpio_core.h>
 /*#include <mach/eint.h>*/
 #include <linux/interrupt.h>
diff --git a/drivers/misc/mediatek/gpio/mt6735/mt_gpio_debug.c b/drivers/misc/mediatek/gpio/mt6735/mt_gpio_debug.c
index 6c080223..6c2a7d5f 100644
--- a/drivers/misc/mediatek/gpio/mt6735/mt_gpio_debug.c
+++ b/drivers/misc/mediatek/gpio/mt6735/mt_gpio_debug.c
@@ -9,7 +9,7 @@
  ******************************************************************************/
 
 #include <linux/slab.h>
-#include <6735_gpio.h>
+#include "6735_gpio.h"
 #include <mt-plat/mt_gpio.h>
 #include <mt-plat/mt_gpio_core.h>
 
diff --git a/drivers/misc/mediatek/gpio/mt6735/mt_gpio_ext.c b/drivers/misc/mediatek/gpio/mt6735/mt_gpio_ext.c
index a35c91ab..99245e11 100644
--- a/drivers/misc/mediatek/gpio/mt6735/mt_gpio_ext.c
+++ b/drivers/misc/mediatek/gpio/mt6735/mt_gpio_ext.c
@@ -10,7 +10,7 @@
 
 #include <mt-plat/mt_gpio.h>
 #include <mt-plat/mt_gpio_core.h>
-#include <mt_gpio_ext.h>
+#include "mt_gpio_ext.h"
 
 /* #define MAX_GPIO_REG_BITS      16 */
 /* #define MAX_GPIO_MODE_PER_REG  5 */
diff --git a/drivers/misc/mediatek/i2c/mt6735/i2c.c b/drivers/misc/mediatek/i2c/mt6735/i2c.c
index 6274df6d..2bc2d4a0 100644
--- a/drivers/misc/mediatek/i2c/mt6735/i2c.c
+++ b/drivers/misc/mediatek/i2c/mt6735/i2c.c
@@ -25,7 +25,7 @@
 #include <asm/io.h>
 /* #include <mach/dma.h> */
 /* #include <mach/mt_reg_base.h> */
-#include <mt_i2c.h>
+#include "mt_i2c.h"
 #include <mt-plat/sync_write.h>
 #include "../../base/power/mt6735/mt_pm_init.h"
 /* #include "mach/memory.h" */
diff --git a/drivers/misc/mediatek/i2c/mt6735/i2c_common.c b/drivers/misc/mediatek/i2c/mt6735/i2c_common.c
index 7e004a7c..abca0d66 100644
--- a/drivers/misc/mediatek/i2c/mt6735/i2c_common.c
+++ b/drivers/misc/mediatek/i2c/mt6735/i2c_common.c
@@ -8,7 +8,7 @@
 #include <linux/err.h>
 /* #include <mach/mt_pm_ldo.h> */
 #include <asm/memory.h>
-#include <mt_i2c.h>
+#include "mt_i2c.h"
 
 static char data_buffer[256 * 4];
 
diff --git a/drivers/misc/mediatek/include/mt-plat/mt6735/include/mach/mt_thermal.h b/drivers/misc/mediatek/include/mt-plat/mt6735/include/mach/mt_thermal.h
index 2fe522b6..a7bedac6 100644
--- a/drivers/misc/mediatek/include/mt-plat/mt6735/include/mach/mt_thermal.h
+++ b/drivers/misc/mediatek/include/mt-plat/mt6735/include/mach/mt_thermal.h
@@ -13,7 +13,7 @@
 #include "mt-plat/sync_write.h"
 #include "mtk_thermal_typedefs.h"
 #include "mt-plat/mtk_mdm_monitor.h"
-#include "mt_gpufreq.h"
+#include "../../../../../drivers/misc/mediatek/base/power/mt6735/mt_gpufreq.h"
 /* #include "mach/mt6575_auxadc_hw.h" */
 
 #if !defined(CONFIG_MTK_LEGACY)
diff --git a/drivers/misc/mediatek/include/mt-plat/sd_misc.h b/drivers/misc/mediatek/include/mt-plat/sd_misc.h
index 7e6768c9..cc5f27a6 100644
--- a/drivers/misc/mediatek/include/mt-plat/sd_misc.h
+++ b/drivers/misc/mediatek/include/mt-plat/sd_misc.h
@@ -10,7 +10,7 @@
 #include <linux/mmc/sd.h>
 #endif
 
-#include <mt_sd.h>
+#include "../../../../mmc/host/mediatek/mt6735/mt_sd.h"
 
 #ifndef FPGA_PLATFORM
 extern void msdc_set_driving(struct msdc_host *host, struct msdc_hw *hw, bool sd_18);
diff --git a/drivers/misc/mediatek/m4u/2.0/m4u_pgtable.h b/drivers/misc/mediatek/m4u/2.0/m4u_pgtable.h
index fce98246..d3f5cad2 100644
--- a/drivers/misc/mediatek/m4u/2.0/m4u_pgtable.h
+++ b/drivers/misc/mediatek/m4u/2.0/m4u_pgtable.h
@@ -1,7 +1,7 @@
 #ifndef __M4U_PGTABLE_H__
 #define __M4U_PGTABLE_H__
 
-#include "m4u_reg.h"
+#include "../mt6735/mt6735/m4u_reg.h"
 
 /* ================================================================= */
 /* 2 level pagetable: pgd -> pte */
diff --git a/drivers/misc/mediatek/m4u/2.0/m4u_v2.h b/drivers/misc/mediatek/m4u/2.0/m4u_v2.h
index 6063d8c8..d28148dd 100644
--- a/drivers/misc/mediatek/m4u/2.0/m4u_v2.h
+++ b/drivers/misc/mediatek/m4u/2.0/m4u_v2.h
@@ -2,7 +2,7 @@
 #define __M4U_V2_H__
 #include <linux/ioctl.h>
 #include <linux/fs.h>
-#include "m4u_port.h"
+#include "../mt6735/m4u_port.h"
 #include <linux/scatterlist.h>
 
 typedef int M4U_PORT_ID;
diff --git a/drivers/misc/mediatek/m4u/mt6735/m4u_priv.h b/drivers/misc/mediatek/m4u/mt6735/m4u_priv.h
index 69dfa34b..7d4554d8 100644
--- a/drivers/misc/mediatek/m4u/mt6735/m4u_priv.h
+++ b/drivers/misc/mediatek/m4u/mt6735/m4u_priv.h
@@ -12,9 +12,9 @@
 #endif
 
 #include "m4u.h"
-#include "m4u_reg.h"
+#include "mt6735/m4u_reg.h"
 #include "../2.0/m4u_pgtable.h"
-#include "m4u_platform.h"
+#include "mt6735/m4u_platform.h"
 
 #define M4UMSG(string, args...)	pr_err("M4U"string, ##args)
 #define M4UINFO(string, args...) pr_debug("M4U"string, ##args)
diff --git a/drivers/misc/mediatek/power/mt6735/mt6311.c b/drivers/misc/mediatek/power/mt6735/mt6311.c
index 018fc81f..9d71d731 100644
--- a/drivers/misc/mediatek/power/mt6735/mt6311.c
+++ b/drivers/misc/mediatek/power/mt6735/mt6311.c
@@ -27,7 +27,7 @@
 /*#include <mach/eint.h> TBD*/
 
 #include <mt-plat/upmu_common.h>
-#include <mt6311.h>
+#include "mt6311.h"
 
 #include <mach/mt_pmic.h>
 
diff --git a/drivers/misc/mediatek/power/mt6735/pmic.c b/drivers/misc/mediatek/power/mt6735/pmic.c
index 132569a5..b3b2f254 100644
--- a/drivers/misc/mediatek/power/mt6735/pmic.c
+++ b/drivers/misc/mediatek/power/mt6735/pmic.c
@@ -65,7 +65,7 @@
 #include <linux/gpio/consumer.h>
 #endif
 #include <mt-plat/upmu_common.h>
-#include <pmic.h>
+#include "pmic.h"
 /*#include <mach/eint.h> TBD*/
 #include <mach/mt_pmic_wrap.h>
 #if defined CONFIG_MTK_LEGACY
@@ -89,7 +89,7 @@
 //#include <mach/mt_battery_meter.h>
 #include "cust_battery_meter.h"
 #endif
-#include <mt6311.h>
+#include "mt6311.h"
 #include <mach/mt_pmic.h>
 
 #include <mt-plat/aee.h>
diff --git a/drivers/misc/mediatek/uart/include/mtk_uart.h b/drivers/misc/mediatek/uart/include/mtk_uart.h
index d971cb0a..e60b128e 100644
--- a/drivers/misc/mediatek/uart/include/mtk_uart.h
+++ b/drivers/misc/mediatek/uart/include/mtk_uart.h
@@ -5,7 +5,7 @@
 #include <mach/mt_reg_base.h>
 #endif
 #include <mt-plat/sync_write.h>
-#include "platform_uart.h"
+#include "../mt6735/platform_uart.h"
 
 /*---------------------------------------------------------------------------*/
 #if defined(ENABLE_VFIFO_DEBUG)
diff --git a/drivers/misc/mediatek/uart/include/mtk_uart_intf.h b/drivers/misc/mediatek/uart/include/mtk_uart_intf.h
index aff13c8a..60321384 100644
--- a/drivers/misc/mediatek/uart/include/mtk_uart_intf.h
+++ b/drivers/misc/mediatek/uart/include/mtk_uart_intf.h
@@ -1,7 +1,7 @@
 #ifndef __MTK_UART_INTF_H__
 #define __MTK_UART_INTF_H__
 
-#include "platform_uart.h"
+#include "../mt6735/platform_uart.h"
 #include <linux/platform_device.h>
 /*---------------------------------------------------------------------------*/
 /* fiq debugger */
diff --git a/drivers/misc/mediatek/video/common/mtkfb_fence.h b/drivers/misc/mediatek/video/common/mtkfb_fence.h
index d8bae158..748c9949 100644
--- a/drivers/misc/mediatek/video/common/mtkfb_fence.h
+++ b/drivers/misc/mediatek/video/common/mtkfb_fence.h
@@ -4,8 +4,8 @@
 #include <linux/mutex.h>
 #include <linux/list.h>
 #include "disp_session.h"
-#include "disp_drv_platform.h"
-#include "display_recorder.h"
+#include "../mt6735/videox/mt6735/disp_drv_platform.h"
+#include "../mt6735/dispsys/display_recorder.h"
 
 #ifdef __cplusplus
 extern "C" {
diff --git a/drivers/misc/mediatek/video/common/rdma10/ddp_rdma.h b/drivers/misc/mediatek/video/common/rdma10/ddp_rdma.h
index 4f4b3ac9..99c1ed6b 100644
--- a/drivers/misc/mediatek/video/common/rdma10/ddp_rdma.h
+++ b/drivers/misc/mediatek/video/common/rdma10/ddp_rdma.h
@@ -4,8 +4,8 @@
 #include <mt-plat/sync_write.h>
 #include <linux/types.h>
 /* #include <mach/mt_reg_base.h> */
-#include "ddp_info.h"
-#include "ddp_hal.h"
+#include "../../mt6735/dispsys/ddp_info.h"
+#include "../../mt6735/dispsys/ddp_hal.h"
 
 extern unsigned long long rdma_start_time[];
 extern unsigned long long rdma_end_time[];
diff --git a/drivers/misc/mediatek/video/common/wdma10/ddp_wdma.h b/drivers/misc/mediatek/video/common/wdma10/ddp_wdma.h
index 78e85172..3728d329 100644
--- a/drivers/misc/mediatek/video/common/wdma10/ddp_wdma.h
+++ b/drivers/misc/mediatek/video/common/wdma10/ddp_wdma.h
@@ -1,8 +1,8 @@
 #ifndef _DDP_WDMA_H_
 #define _DDP_WDMA_H_
 
-#include "ddp_hal.h"
-#include "ddp_info.h"
+#include "../../mt6735/dispsys/ddp_hal.h"
+#include "../../mt6735/dispsys/ddp_info.h"
 
 /* start module */
 int wdma_start(DISP_MODULE_ENUM module, void *handle);
diff --git a/drivers/misc/mediatek/video/mt6735/dispsys/ddp_pwm_mux.c b/drivers/misc/mediatek/video/mt6735/dispsys/ddp_pwm_mux.c
index f86dfb42..759eee39 100644
--- a/drivers/misc/mediatek/video/mt6735/dispsys/ddp_pwm_mux.c
+++ b/drivers/misc/mediatek/video/mt6735/dispsys/ddp_pwm_mux.c
@@ -1,10 +1,10 @@
 #include <linux/kernel.h>
 #include <linux/clk.h>
-#include <ddp_drv.h>
-#include <ddp_pwm_mux.h>
+#include "ddp_drv.h"
+#include "../../include/ddp_pwm_mux.h"
 #include <linux/of.h>
 #include <linux/of_address.h>
-#include <ddp_reg.h>
+#include "mt6735/ddp_reg.h"
 
 #define PWM_MSG(fmt, arg...) pr_debug("[PWM] " fmt "\n", ##arg)
 #define PWM_ERR(fmt, arg...) pr_err("[PWM] " fmt "\n", ##arg)
diff --git a/drivers/misc/mediatek/video/mt6735/dispsys/mt6735/ddp_ovl.h b/drivers/misc/mediatek/video/mt6735/dispsys/mt6735/ddp_ovl.h
index 7a8c5dc8..8dad5b89 100644
--- a/drivers/misc/mediatek/video/mt6735/dispsys/mt6735/ddp_ovl.h
+++ b/drivers/misc/mediatek/video/mt6735/dispsys/mt6735/ddp_ovl.h
@@ -1,9 +1,9 @@
 #ifndef _DDP_OVL_H_
 #define _DDP_OVL_H_
 
-#include "ddp_hal.h"
+#include "../ddp_hal.h"
 #include "DpDataType.h"
-#include "ddp_info.h"
+#include "../ddp_info.h"
 
 
 #define OVL_MAX_WIDTH  (4095)
diff --git a/drivers/misc/mediatek/video/mt6735/dispsys/mt6735/ddp_rdma_ex.h b/drivers/misc/mediatek/video/mt6735/dispsys/mt6735/ddp_rdma_ex.h
index 80e16a42..f934000f 100644
--- a/drivers/misc/mediatek/video/mt6735/dispsys/mt6735/ddp_rdma_ex.h
+++ b/drivers/misc/mediatek/video/mt6735/dispsys/mt6735/ddp_rdma_ex.h
@@ -1,6 +1,6 @@
 #ifndef _DDP_RDMA_EX_H_
 #define _DDP_RDMA_EX_H_
-#include "ddp_info.h"
+#include "../ddp_info.h"
 
 #define RDMA_INSTANCES  2
 #define RDMA_MAX_WIDTH  4095
diff --git a/drivers/misc/mediatek/video/mt6735/dispsys/mt6735/ddp_reg.h b/drivers/misc/mediatek/video/mt6735/dispsys/mt6735/ddp_reg.h
index c40eec43..6dd2bb7f 100644
--- a/drivers/misc/mediatek/video/mt6735/dispsys/mt6735/ddp_reg.h
+++ b/drivers/misc/mediatek/video/mt6735/dispsys/mt6735/ddp_reg.h
@@ -3,11 +3,11 @@
 #include <mt-plat/sync_write.h>
 /* #include <mach/mt_reg_base.h> */
 #include <linux/types.h>
-#include "display_recorder.h"
-#include "cmdq_record.h"
-#include "cmdq_core.h"
-#include "ddp_hal.h"
-#include "ddp_log.h"
+#include "../display_recorder.h"
+#include "../../../../cmdq/v2/cmdq_record.h"
+#include "../../../../cmdq/v2/cmdq_core.h"
+#include "../ddp_hal.h"
+#include "../ddp_log.h"
 
 /* MIPITX and DSI */
 #define ENABLE_CLK_MGR
diff --git a/drivers/misc/mediatek/video/mt6735/videox/disp_drv_log.h b/drivers/misc/mediatek/video/mt6735/videox/disp_drv_log.h
index 4262d8be..d2fa28b7 100644
--- a/drivers/misc/mediatek/video/mt6735/videox/disp_drv_log.h
+++ b/drivers/misc/mediatek/video/mt6735/videox/disp_drv_log.h
@@ -1,8 +1,8 @@
 #ifndef __DISP_DRV_LOG_H__
 #define __DISP_DRV_LOG_H__
-#include "display_recorder.h"
-#include "ddp_debug.h"
-#include "disp_drv_platform.h"
+#include "../dispsys/display_recorder.h"
+#include "../dispsys/ddp_debug.h"
+#include "mt6735/disp_drv_platform.h"
 
 extern unsigned int dprec_error_log_len;
 extern unsigned int dprec_error_log_id;
diff --git a/drivers/misc/mediatek/video/mt6735/videox/mt6735/disp_drv_platform.h b/drivers/misc/mediatek/video/mt6735/videox/mt6735/disp_drv_platform.h
index a359f009..a52314e0 100644
--- a/drivers/misc/mediatek/video/mt6735/videox/mt6735/disp_drv_platform.h
+++ b/drivers/misc/mediatek/video/mt6735/videox/mt6735/disp_drv_platform.h
@@ -15,10 +15,10 @@
 /*#include <board-custom.h>*/
 #include "disp_assert_layer.h"
 #include <mt-plat/sync_write.h>
-#include "ddp_hal.h"
+#include "../../dispsys/ddp_hal.h"
 /* #include "ddp_drv.h" */
-#include "ddp_path.h"
-#include "ddp_ovl.h"
+#include "../../dispsys/ddp_path.h"
+#include "../../dispsys/mt6735/ddp_ovl.h"
 
 
 #define ALIGN_TO(x, n)  \
diff --git a/drivers/misc/mediatek/video/mt6735/videox/primary_display.h b/drivers/misc/mediatek/video/mt6735/videox/primary_display.h
index 673ff8df..35ea98aa 100644
--- a/drivers/misc/mediatek/video/mt6735/videox/primary_display.h
+++ b/drivers/misc/mediatek/video/mt6735/videox/primary_display.h
@@ -1,8 +1,8 @@
 #ifndef _PRIMARY_DISPLAY_H_
 #define _PRIMARY_DISPLAY_H_
 
-#include "ddp_hal.h"
-#include "ddp_manager.h"
+#include "../dispsys/ddp_hal.h"
+#include "../dispsys/ddp_manager.h"
 #include <linux/types.h>
 #include "disp_lcm.h"
 #include "disp_session.h"
diff --git a/drivers/watchdog/mediatek/wdt/mt6735/mtk_wdt.c b/drivers/watchdog/mediatek/wdt/mt6735/mtk_wdt.c
index 9d6869ba..93fb16a3 100644
--- a/drivers/watchdog/mediatek/wdt/mt6735/mtk_wdt.c
+++ b/drivers/watchdog/mediatek/wdt/mt6735/mtk_wdt.c
@@ -11,7 +11,7 @@
 
 #include <asm/uaccess.h>
 #include <linux/types.h>
-#include <mt_wdt.h>
+#include "mt_wdt.h"
 #include <linux/delay.h>
 
 #include <linux/device.h>
diff --git a/kernel/power/tuxonice_ui.c b/kernel/power/tuxonice_ui.c
index fc3ac655..cdcc531c 100644
--- a/kernel/power/tuxonice_ui.c
+++ b/kernel/power/tuxonice_ui.c
@@ -124,7 +124,7 @@ void toi_early_boot_message(int message_detail, int default_answer, char *warnin
 		say("BIG FAT WARNING!! %s", local_printf_buf);
 		switch (message_detail) {
 		case 0:
-			say("If you continue booting, note that any image WILL NOT BE REMOVED")
+			say("If you continue booting, note that any image WILL NOT BE REMOVED");
 			/* TuxOnIce is unable to do so because the appropriate modules aren't loaded.
 			 * You should manually remove the image to avoid any possibility of corrupting
 			 * your filesystem(s) later.
diff --git a/kernel/power/tuxonice_userui.c b/kernel/power/tuxonice_userui.c
index 77e0a37c..faf19196 100644
--- a/kernel/power/tuxonice_userui.c
+++ b/kernel/power/tuxonice_userui.c
@@ -315,10 +315,10 @@ static void userui_prepare_status(int clearbar, const char *fmt, ...)
 	if (clearbar)
 		toi_update_status(0, 1, NULL);
 
-	if (ui_helper_data.pid == -1)
+	//if (ui_helper_data.pid == -1)
 		pr_err("%s\n", lastheader);
-	else
-		toi_message(0, TOI_STATUS, 1, lastheader, NULL);
+	//else
+	//	toi_message(0, TOI_STATUS, 1, lastheader, NULL);
 }
 
 /**
diff --git a/drivers/misc/mediatek/video/mt6735/videox/mt6735/disp_drv_platform.h b/drivers/misc/mediatek/video/mt6735/videox/mt6735/disp_drv_platform.h
index a52314e0..1e42b6c6 100644
--- a/drivers/misc/mediatek/video/mt6735/videox/mt6735/disp_drv_platform.h
+++ b/drivers/misc/mediatek/video/mt6735/videox/mt6735/disp_drv_platform.h
@@ -13,7 +13,7 @@
 #endif
 /* #include <mach/mt_irq.h> */
 /*#include <board-custom.h>*/
-#include "disp_assert_layer.h"
+#include "../disp_assert_layer.h"
 #include <mt-plat/sync_write.h>
 #include "../../dispsys/ddp_hal.h"
 /* #include "ddp_drv.h" */
diff --git a/drivers/pinctrl/mediatek/pinctrl-mtk-mt6735.h b/drivers/pinctrl/mediatek/pinctrl-mtk-mt6735.h
index 4bc6b34d..280ecd16 100644
--- a/drivers/pinctrl/mediatek/pinctrl-mtk-mt6735.h
+++ b/drivers/pinctrl/mediatek/pinctrl-mtk-mt6735.h
@@ -12,7 +12,7 @@
 #define __PINCTRL_MTK_MT6735_H
 
 #include <linux/pinctrl/pinctrl.h>
-#include <pinctrl-mtk-common.h>
+#include "pinctrl-mtk-common.h"
 
 static const struct mtk_desc_pin mtk_pins_mt6735[] = {
 	MTK_PIN(
diff --git a/drivers/spi/mediatek/mt6735/spi.c b/drivers/spi/mediatek/mt6735/spi.c
index c5cfe271..0b832910 100644
--- a/drivers/spi/mediatek/mt6735/spi.c
+++ b/drivers/spi/mediatek/mt6735/spi.c
@@ -27,7 +27,7 @@
 #include <linux/of_address.h>
 #endif
 /*#include <mach/irqs.h>*/
-#include <mt_spi.h>
+#include "mt_spi.h"
 #include "mt_spi_hal.h"
 /*#include <mach/mt_gpio.h>*/
 
diff --git a/drivers/spi/mediatek/mt6735/spi-dev.c b/drivers/spi/mediatek/mt6735/spi-dev.c
index 1408ae3b..3c1075cd 100644
--- a/drivers/spi/mediatek/mt6735/spi-dev.c
+++ b/drivers/spi/mediatek/mt6735/spi-dev.c
@@ -4,7 +4,7 @@
 #include <linux/types.h>
 #include <linux/device.h>
 #include <linux/delay.h>
-#include <mt_spi.h>
+#include "mt_spi.h"
 
 #include <linux/dma-mapping.h>
 #include <linux/sched.h>
