# Archived: Downstream port, only for testing. Use mainline port!
# Reference: <https://postmarketos.org/devicepkg>
pkgname=device-motorola-falcon-downstream
pkgdesc="Moto G (2013) (Downstream)"
pkgver=3
pkgrel=0
url="https://postmarketos.org"
license="MIT"
arch="armv7"
options="!check !archcheck"
depends="
	firmware-motorola-falcon
	linux-motorola-falcon-downstream
	mkbootimg
	msm-fb-refresher
	postmarketos-base
	"
makedepends="devicepkg-dev"
source="
	deviceinfo
	kernel-cmdline.conf
	"

build() {
	devicepkg_build $startdir $pkgname
}

package() {
	devicepkg_package $startdir $pkgname
}

sha512sums="
bf5f275fe8bb4b814a2a82614ac58256756f60e5eae1e8df02102367144a02b649417b0b24c170c8b21ad957c899e56b26dd40b553b22b1fe6e8f1d6297c4bbd  deviceinfo
041616fe111ac217376660feb5a9e57550f585f59033e84d4550679ac150cdb827da17d9cdb65580b23e11170ed751f8e1d77c2830a16bb9e5aadea9a83f0320  kernel-cmdline.conf
"
