#!/stage1/busybox sh

# Samsung kernels come with their own initramfs, which extract and load another
# initramfs. Usually that depends on the recovery key combination being pressed
# or not. For simplicity, we always boot the recovery image (from the kernel2
# partition) here.

_PATH="$PATH"
export PATH=/stage1

busybox cd /
busybox date >>boot.txt
exec >>boot.txt 2>&1
busybox rm init
busybox mount -t proc proc /proc
busybox mount -t sysfs sysfs /sys

# always use the "isorec"-style lzop compressed initramfs
# from the kernel2 partition
load_image=/stage1/isorec.cpio
busybox lzop -dc /dev/block/mmcblk0p17 > ${load_image}
busybox cpio -i < ${load_image}

busybox umount /sys
busybox umount /proc
busybox date >>boot.txt
busybox rm -fr /stage1 /dev/*
export PATH="${_PATH}"
exec /init
