# Archived: unmaintained port, only for testing. Use generic/mainline port (qcom-msm8953)
pkgname=firmware-xiaomi-rosy
pkgver=1
pkgrel=1
pkgdesc="Firmware files for Xiaomi Redmi 5"
url="https://gitlab.com/barni2000/$pkgname"
arch="aarch64"
license="proprietary"
options="!strip !check !archcheck !spdx !tracedeps pmb:cross-native"

_commit="69c6d964bc0034bd93292286ac101c23fc804d72"

source="$pkgname-$_commit.tar.gz::$url/-/archive/$_commit/$pkgname-$_commit.tar.gz"
builddir="$srcdir/$pkgname-$_commit"

_fwdir="/lib/firmware/qcom/msm8953/xiaomi/rosy"

package() {
	install -Dm644 a506_zap.b02 -t "$pkgdir/$_fwdir"
	install -Dm644 a506_zap.mdt -t "$pkgdir/$_fwdir"
}

sha512sums="
e1f0cd1383ba95cef08236dc470e4be05852387152be7772488f423f5a2e9ec1f7b27203ebf1e3bcb98b3998387b510546ebdcb81b0137a180912c67b850cc07  firmware-xiaomi-rosy-69c6d964bc0034bd93292286ac101c23fc804d72.tar.gz
"
