# Default is to use /dev/rtc0, which uses the S3C RTC on Samsung
# Manta, and somehow does not work.
# Use /dev/rtc1 instead, which uses the MAX77686 RTC, and works
# without issues.
clock_args="-f /dev/rtc1"
