diff --git a/arch/arm64/boot/dts/amlogic/Makefile b/arch/arm64/boot/dts/amlogic/Makefile
index cc8b34bd5..758d5d3ad 100644
--- a/arch/arm64/boot/dts/amlogic/Makefile
+++ b/arch/arm64/boot/dts/amlogic/Makefile
@@ -12,6 +12,7 @@ dtb-$(CONFIG_ARCH_MESON) += meson-g12a-radxa-zero.dtb
 dtb-$(CONFIG_ARCH_MESON) += meson-g12a-sei510.dtb
 dtb-$(CONFIG_ARCH_MESON) += meson-g12a-u200.dtb
 dtb-$(CONFIG_ARCH_MESON) += meson-g12a-x96-max.dtb
+dtb-$(CONFIG_ARCH_MESON) += meson-g12a-b860hv5.dtb
 dtb-$(CONFIG_ARCH_MESON) += meson-g12b-a311d-bananapi-m2s.dtb
 dtb-$(CONFIG_ARCH_MESON) += meson-g12b-a311d-khadas-vim3.dtb
 dtb-$(CONFIG_ARCH_MESON) += meson-g12b-bananapi-cm4-cm4io.dtb
diff --git a/arch/arm64/boot/dts/amlogic/meson-g12a-b860hv5.dts b/arch/arm64/boot/dts/amlogic/meson-g12a-b860hv5.dts
new file mode 100644
index 000000000..68c9360a5
--- /dev/null
+++ b/arch/arm64/boot/dts/amlogic/meson-g12a-b860hv5.dts
@@ -0,0 +1,491 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Copyright (c) 2018 BayLibre SAS. All rights reserved.
+ *
+ */
+
+/dts-v1/;
+
+#include "meson-g12a.dtsi"
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/gpio/meson-g12a-gpio.h>
+#include <dt-bindings/sound/meson-g12a-tohdmitx.h>
+
+/ {
+       compatible = "amlogic,g12a";
+       model = "ZTE B860H V5";
+
+       aliases {
+               serial0 = &uart_AO;
+               ethernet0 = &ethmac;
+       };
+
+       spdif_dit: audio-codec-1 {
+               #sound-dai-cells = <0>;
+               compatible = "linux,spdif-dit";
+               sound-name-prefix = "DIT";
+       };
+
+       chosen {
+               stdout-path = "serial0:115200n8";
+       };
+
+       memory@0 {
+               device_type = "memory";
+               reg = <0x0 0x0 0x0 0x80000000>;
+       };
+
+       cvbs-connector {
+               compatible = "composite-video-connector";
+
+               port {
+                       cvbs_connector_in: endpoint {
+                               remote-endpoint = <&cvbs_vdac_out>;
+                       };
+               };
+       };
+
+       hdmi-connector {
+               compatible = "hdmi-connector";
+               type = "a";
+
+               port {
+                       hdmi_connector_in: endpoint {
+                               remote-endpoint = <&hdmi_tx_tmds_out>;
+                       };
+               };
+       };
+
+       emmc_pwrseq: emmc-pwrseq {
+               compatible = "mmc-pwrseq-emmc";
+               reset-gpios = <&gpio BOOT_12 GPIO_ACTIVE_LOW>;
+       };
+
+       sdio_pwrseq: sdio-pwrseq {
+               compatible = "mmc-pwrseq-simple";
+               reset-gpios = <&gpio GPIOX_6 GPIO_ACTIVE_LOW>;
+               clocks = <&wifi32k>;
+               clock-names = "ext_clock";
+       };
+
+       flash_1v8: regulator-flash_1v8 {
+               compatible = "regulator-fixed";
+               regulator-name = "FLASH_1V8";
+               regulator-min-microvolt = <1800000>;
+               regulator-max-microvolt = <1800000>;
+               vin-supply = <&vcc_3v3>;
+               regulator-always-on;
+       };
+
+       dc_in: regulator-dc_in {
+               compatible = "regulator-fixed";
+               regulator-name = "DC_IN";
+               regulator-min-microvolt = <5000000>;
+               regulator-max-microvolt = <5000000>;
+               regulator-always-on;
+       };
+
+       vcc_1v8: regulator-vcc_1v8 {
+               compatible = "regulator-fixed";
+               regulator-name = "VCC_1V8";
+               regulator-min-microvolt = <1800000>;
+               regulator-max-microvolt = <1800000>;
+               vin-supply = <&vcc_3v3>;
+               regulator-always-on;
+       };
+
+       vcc_3v3: regulator-vcc_3v3 {
+               compatible = "regulator-fixed";
+               regulator-name = "VCC_3V3";
+               regulator-min-microvolt = <3300000>;
+               regulator-max-microvolt = <3300000>;
+               vin-supply = <&vddao_3v3>;
+               regulator-always-on;
+               /* FIXME: actually controlled by VDDCPU_B_EN */
+       };
+
+       vcc_5v: regulator-vcc_5v {
+               compatible = "regulator-fixed";
+               regulator-name = "VCC_5V";
+               regulator-min-microvolt = <5000000>;
+               regulator-max-microvolt = <5000000>;
+               vin-supply = <&dc_in>;
+
+               gpio = <&gpio GPIOH_8 GPIO_OPEN_DRAIN>;
+       };
+
+       vddao_1v8: regulator-vddao_1v8 {
+               compatible = "regulator-fixed";
+               regulator-name = "VDDAO_1V8";
+               regulator-min-microvolt = <1800000>;
+               regulator-max-microvolt = <1800000>;
+               vin-supply = <&vddao_3v3>;
+               regulator-always-on;
+       };
+
+       vddao_3v3: regulator-vddao_3v3 {
+               compatible = "regulator-fixed";
+               regulator-name = "VDDAO_3V3";
+               regulator-min-microvolt = <3300000>;
+               regulator-max-microvolt = <3300000>;
+               vin-supply = <&dc_in>;
+               regulator-always-on;
+       };
+
+       vddcpu: regulator-vddcpu {
+               compatible = "pwm-regulator";
+
+               regulator-name = "VDDCPU";
+               regulator-min-microvolt = <721000>;
+               regulator-max-microvolt = <1022000>;
+
+               pwm-supply = <&dc_in>;
+
+               pwms = <&pwm_AO_cd 1 1250 0>;
+               pwm-dutycycle-range = <100 0>;
+
+               regulator-boot-on;
+               regulator-always-on;
+       };
+
+       vddgpu: regulator-vddgpu {
+               compatible = "regulator-fixed";
+               regulator-name = "mali";
+               regulator-min-microvolt = <800000>;
+               regulator-max-microvolt = <800000>;
+               vin-supply = <&dc_in>;
+               regulator-boot-on;
+               regulator-always-on;
+       };
+
+       sound {
+               dai-link-0 {
+                       sound-dai = <&frddr_a>;
+               };
+
+               dai-link-1 {
+                       sound-dai = <&frddr_b>;
+               };
+
+               dai-link-2 {
+                       sound-dai = <&frddr_c>;
+               };
+
+               /* 8ch hdmi interface */
+               dai-link-3 {
+                       sound-dai = <&tdmif_b>;
+                       dai-format = "i2s";
+                       dai-tdm-slot-tx-mask-0 = <1 1>;
+                       dai-tdm-slot-tx-mask-1 = <1 1>;
+                       dai-tdm-slot-tx-mask-2 = <1 1>;
+                       dai-tdm-slot-tx-mask-3 = <1 1>;
+                       mclk-fs = <256>;
+
+                       codec {
+                               sound-dai = <&tohdmitx TOHDMITX_I2S_IN_B>;
+                       };
+               };
+
+               /* hdmi glue */
+               dai-link-6 {
+                       sound-dai = <&tohdmitx TOHDMITX_I2S_OUT>;
+
+                       codec {
+                               sound-dai = <&hdmi_tx>;
+                       };
+               };
+       };
+
+       wifi32k: wifi32k {
+               compatible = "pwm-clock";
+               #clock-cells = <0>;
+               clock-frequency = <32768>;
+               pwms = <&pwm_ef 0 30518 0>; /* PWM_E at 32.768KHz */
+       };
+};
+
+&arb {
+       status = "okay";
+};
+
+&cec_AO {
+       pinctrl-0 = <&cec_ao_a_h_pins>;
+       pinctrl-names = "default";
+       status = "disabled";
+       hdmi-phandle = <&hdmi_tx>;
+};
+
+&cecb_AO {
+       pinctrl-0 = <&cec_ao_b_h_pins>;
+       pinctrl-names = "default";
+       status = "okay";
+       hdmi-phandle = <&hdmi_tx>;
+};
+
+&clkc_audio {
+       status = "okay";
+};
+
+&cpu0 {
+       cpu-supply = <&vddcpu>;
+       operating-points-v2 = <&cpu_opp_table>;
+       clocks = <&clkc CLKID_CPU_CLK>;
+       clock-latency = <50000>;
+};
+
+&cpu1 {
+       cpu-supply = <&vddcpu>;
+       operating-points-v2 = <&cpu_opp_table>;
+       clocks = <&clkc CLKID_CPU_CLK>;
+       clock-latency = <50000>;
+};
+
+&cpu2 {
+       cpu-supply = <&vddcpu>;
+       operating-points-v2 = <&cpu_opp_table>;
+       clocks = <&clkc CLKID_CPU_CLK>;
+       clock-latency = <50000>;
+};
+
+&cpu3 {
+       cpu-supply = <&vddcpu>;
+       operating-points-v2 = <&cpu_opp_table>;
+       clocks = <&clkc CLKID_CPU_CLK>;
+       clock-latency = <50000>;
+};
+
+&mali {
+       mali-supply = <&vddgpu>;
+};
+
+&cvbs_vdac_port {
+       cvbs_vdac_out: endpoint {
+               remote-endpoint = <&cvbs_connector_in>;
+       };
+};
+
+&frddr_a {
+       status = "okay";
+};
+
+&frddr_b {
+       status = "okay";
+};
+
+&frddr_c {
+       status = "okay";
+};
+
+&hdmi_tx {
+       status = "okay";
+       pinctrl-0 = <&hdmitx_hpd_pins>, <&hdmitx_ddc_pins>;
+       pinctrl-names = "default";
+       hdmi-supply = <&vcc_5v>;
+};
+
+&hdmi_tx_tmds_port {
+       hdmi_tx_tmds_out: endpoint {
+               remote-endpoint = <&hdmi_connector_in>;
+       };
+};
+
+&ir {
+       status = "okay";
+       pinctrl-0 = <&remote_input_ao_pins>;
+       pinctrl-names = "default";
+       linux,rc-map-name = "rc-aml";
+};
+
+&pwm_AO_cd {
+       pinctrl-0 = <&pwm_ao_d_e_pins>;
+       pinctrl-names = "default";
+       clocks = <&xtal>;
+       clock-names = "clkin1";
+       status = "okay";
+};
+
+&ext_mdio {
+       external_phy: ethernet-phy@0 {
+               /* Realtek RTL8211F (0x001cc916) */
+               reg = <0>;
+               max-speed = <1000>;
+               eee-broken-1000t;
+
+               reset-assert-us = <10000>;
+               reset-deassert-us = <80000>;
+               reset-gpios = <&gpio GPIOZ_15 (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
+
+               interrupt-parent = <&gpio_intc>;
+               /* MAC_INTR on GPIOZ_14 */
+               interrupts = <26 IRQ_TYPE_LEVEL_LOW>;
+       };
+};
+
+&ethmac {
+       pinctrl-0 = <&eth_pins>;
+       pinctrl-names = "default";
+       status = "okay";
+       phy-mode = "rmii";
+       phy-handle = <&internal_ephy>;
+};
+
+&pwm_ef {
+       status = "okay";
+       pinctrl-0 = <&pwm_e_pins>;
+       pinctrl-names = "default";
+       clocks = <&xtal>;
+       clock-names = "clkin0";
+};
+
+&uart_A {
+       status = "okay";
+       pinctrl-0 = <&uart_a_pins>, <&uart_a_cts_rts_pins>;
+       pinctrl-names = "default";
+       uart-has-rtscts;
+
+       bluetooth {
+               compatible = "brcm,bcm43438-bt";
+               shutdown-gpios = <&gpio GPIOX_17 GPIO_ACTIVE_HIGH>;
+               max-speed = <2000000>;
+               clocks = <&wifi32k>;
+               clock-names = "lpo";
+       };
+};
+
+&uart_AO {
+       status = "okay";
+       pinctrl-0 = <&uart_ao_a_pins>;
+       pinctrl-names = "default";
+};
+
+&usb {
+       status = "okay";
+};
+
+/* SDIO */
+&sd_emmc_a {
+       status = "okay";
+       pinctrl-0 = <&sdio_pins>;
+       pinctrl-1 = <&sdio_clk_gate_pins>;
+       pinctrl-names = "default", "clk-gate";
+       #address-cells = <1>;
+       #size-cells = <0>;
+
+       bus-width = <4>;
+       cap-sd-highspeed;
+       sd-uhs-sdr104;
+       max-frequency = <200000000>;
+
+       non-removable;
+       disable-wp;
+
+       /* WiFi firmware requires power to be kept while in suspend */
+       keep-power-in-suspend;
+
+       mmc-pwrseq = <&sdio_pwrseq>;
+
+       vmmc-supply = <&vddao_3v3>;
+       vqmmc-supply = <&vddao_1v8>;
+};
+
+/* SD card */
+&sd_emmc_b {
+       status = "okay";
+       pinctrl-0 = <&sdcard_c_pins>;
+       pinctrl-1 = <&sdcard_clk_gate_c_pins>;
+       pinctrl-names = "default", "clk-gate";
+
+       bus-width = <4>;
+       cap-sd-highspeed;
+       max-frequency = <50000000>;
+       disable-wp;
+
+       cd-gpios = <&gpio GPIOC_6 GPIO_ACTIVE_LOW>;
+       vmmc-supply = <&vddao_3v3>;
+       vqmmc-supply = <&vddao_3v3>;
+};
+
+/* eMMC */
+&sd_emmc_c {
+       status = "okay";
+       pinctrl-0 = <&emmc_ctrl_pins>, <&emmc_data_8b_pins>, <&emmc_ds_pins>;
+       pinctrl-1 = <&emmc_clk_gate_pins>;
+       pinctrl-names = "default", "clk-gate";
+
+       bus-width = <8>;
+       cap-mmc-highspeed;
+       mmc-ddr-1_8v;
+       mmc-hs200-1_8v;
+       max-frequency = <200000000>;
+       non-removable;
+       disable-wp;
+
+       mmc-pwrseq = <&emmc_pwrseq>;
+       vmmc-supply = <&vcc_3v3>;
+       vqmmc-supply = <&flash_1v8>;
+};
+
+&tdmif_b {
+       status = "okay";
+};
+
+&tdmout_b {
+       status = "okay";
+};
+
+&tohdmitx {
+       status = "okay";
+};
+
+&cpu_opp_table {
+       opp-1908000000 {
+               opp-hz = /bits/ 64 <1908000000>;
+               opp-microvolt = <1021000>;
+       };
+};
+
+&efuse {
+       eth_mac: eth_mac@0 {
+               reg = <0x0 0x06>;
+       };
+
+       bt_mac: bt_mac@6 {
+               reg = <0x6 0x06>;
+       };
+
+       wifi_mac: wifi_mac@12 {
+               reg = <0x0c 0x06>;
+       };
+
+       usid: usid@18 {
+               reg = <0x12 0x10>;
+       };
+};
+
+&cpu_opp_table {
+       opp-100000000 {
+               status = "disabled";
+       };
+
+       opp-250000000 {
+               status = "disabled";
+       };
+
+       opp-500000000 {
+               status = "disabled";
+       };
+
+       opp-667000000 {
+               status = "disabled";
+       };
+
+       opp-1908000000 {
+               opp-hz = /bits/ 64 <1908000000>;
+               opp-microvolt = <1001000>;
+       };
+
+       opp-2016000000 {
+                       opp-hz = /bits/ 64 <2016000000>;
+                       opp-microvolt = <1021000>;
+       };
+};
