From 3cab66ec47c0691a9dbd8117766055b5e5bec874 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Duje=20Mihanovi=C4=87?= <duje@dujemihanovic.xyz>
Date: Sat, 13 Sep 2025 23:21:09 +0200
Subject: [PATCH 10/21] arm64: dts: marvell: samsung,coreprimevelte: Drop some
 reserved memory
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Most of the memory marked as reserved is actually usable. Delete its
reserved-memory nodes so that the memory can be used.

Signed-off-by: Duje Mihanović <duje@dujemihanovic.xyz>
---
 .../mmp/pxa1908-samsung-coreprimevelte.dts      | 17 -----------------
 1 file changed, 17 deletions(-)

diff --git a/arch/arm64/boot/dts/marvell/mmp/pxa1908-samsung-coreprimevelte.dts b/arch/arm64/boot/dts/marvell/mmp/pxa1908-samsung-coreprimevelte.dts
index e78e176575ef..2f4f052ad890 100644
--- a/arch/arm64/boot/dts/marvell/mmp/pxa1908-samsung-coreprimevelte.dts
+++ b/arch/arm64/boot/dts/marvell/mmp/pxa1908-samsung-coreprimevelte.dts
@@ -42,23 +42,6 @@ framebuffer@17000000 {
 			reg = <0 0x17000000 0 0x1800000>;
 			no-map;
 		};
-
-		gpu@9000000 {
-			reg = <0 0x9000000 0 0x1000000>;
-		};
-
-		/* Communications processor, aka modem */
-		cp@5000000 {
-			reg = <0 0x5000000 0 0x3000000>;
-		};
-
-		cm3@a000000 {
-			reg = <0 0xa000000 0 0x80000>;
-		};
-
-		seclog@8000000 {
-			reg = <0 0x8000000 0 0x100000>;
-		};
 	};
 
 	i2c-muic {
-- 
2.52.0

