# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="PINE64 PinePhone"
deviceinfo_manufacturer="PINE64"
deviceinfo_codename="pine64-pinephone"
deviceinfo_year="2019"
deviceinfo_dtb="allwinner/sun50i-a64-pinephone-1.1 allwinner/sun50i-a64-pinephone-1.2"
# gpio_vibra: needed for osk-sdl haptic feedback
deviceinfo_arch="aarch64"

# Device related
deviceinfo_drm="true"
deviceinfo_chassis="handset"
deviceinfo_external_storage="true"
deviceinfo_screen_width="720"
deviceinfo_screen_height="1440"
deviceinfo_getty="ttyS0;115200"
deviceinfo_dev_internal_storage="/dev/mmcblk2"
deviceinfo_dev_internal_storage_repartition="true"

# Bootloader related
deviceinfo_sd_embed_firmware="u-boot/pine64-pinephone/u-boot-sunxi-with-spl-528.bin:8"
deviceinfo_partition_type="msdos"
