From fac558fd44fd91425797a2e337b6ef0e451a1c1d Mon Sep 17 00:00:00 2001
From: realaravinth <realaravinth@batsense.net>
Date: Wed, 1 Jul 2020 14:49:18 +0530
Subject: [PATCH] sprd,sc-id replaced with qcom,msm-id

---
 arch/arm/boot/dts/sprd-scx35_gtel3g_rev00.dts | 2 +-
 arch/arm/boot/dts/sprd-scx35_gtel3g_rev01.dts | 2 +-
 arch/arm/boot/dts/sprd-scx35_gtel3g_rev02.dts | 2 +-
 arch/arm/boot/dts/sprd-scx35_gtel3g_rev03.dts | 2 +-
 arch/arm/boot/dts/sprd-scx35_gtel3g_rev04.dts | 2 +-
 arch/arm/boot/dts/sprd-scx35_gtel3g_rev05.dts | 2 +-
 arch/arm/boot/dts/sprd-scx35_gtel3g_rev06.dts | 2 +-
 arch/arm/boot/dts/sprd-scx35_gtel3g_rev07.dts | 2 +-
 arch/arm/boot/dts/sprd-scx35_gtel3g_rev08.dts | 2 +-
 arch/arm/boot/dts/sprd-scx35_gtel3g_rev09.dts | 2 +-
 arch/arm/boot/dts/sprd-scx35_gtel3g_rev10.dts | 2 +-
 arch/arm/boot/dts/sprd-scx35_gtel3g_rev11.dts | 2 +-
 12 files changed, 12 insertions(+), 12 deletions(-)

diff --git a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev00.dts b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev00.dts
index 25ad2efa..b341f365 100755
--- a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev00.dts
+++ b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev00.dts
@@ -27,7 +27,7 @@
 
 / {
 	model = "Spreadtrum SP7730G board";
-        sprd,sc-id = <8830 0 0x20000>;
+        qcom,msm-id = <8830 0 0x20000>;
 	chosen {
 		bootargs = "init=/init root=/dev/ram0 rw";
 		linux,initrd-start = <0x85500000>;
diff --git a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev01.dts b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev01.dts
index 177ece29..b0ddae88 100755
--- a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev01.dts
+++ b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev01.dts
@@ -27,7 +27,7 @@
 
 / {
 	model = "Spreadtrum SP7730G board";
-        sprd,sc-id = <8830 1 0x20000>;
+        qcom,msm-id = <8830 1 0x20000>;
 	chosen {
 		bootargs = "init=/init root=/dev/ram0 rw";
 		linux,initrd-start = <0x85500000>;
diff --git a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev02.dts b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev02.dts
index cf050ab7..8ac7178e 100755
--- a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev02.dts
+++ b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev02.dts
@@ -27,7 +27,7 @@
 
 / {
 	model = "Spreadtrum SP7730G board";
-        sprd,sc-id = <8830 2 0x20000>;
+        qcom,msm-id = <8830 2 0x20000>;
 	chosen {
 		bootargs = "init=/init root=/dev/ram0 rw";
 		linux,initrd-start = <0x85500000>;
diff --git a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev03.dts b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev03.dts
index fc72c8f5..76926108 100755
--- a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev03.dts
+++ b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev03.dts
@@ -27,7 +27,7 @@
 
 / {
 	model = "Spreadtrum SP7730G board";
-        sprd,sc-id = <8830 3 0x20000>;
+        qcom,msm-id = <8830 3 0x20000>;
 	chosen {
 		bootargs = "init=/init root=/dev/ram0 rw";
 		linux,initrd-start = <0x85500000>;
diff --git a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev04.dts b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev04.dts
index 5c5e75a8..449ce412 100755
--- a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev04.dts
+++ b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev04.dts
@@ -27,7 +27,7 @@
 
 / {
 	model = "Spreadtrum SP7730G board";
-        sprd,sc-id = <8830 4 0x20000>;
+        qcom,msm-id = <8830 4 0x20000>;
 	chosen {
 		bootargs = "init=/init root=/dev/ram0 rw";
 		linux,initrd-start = <0x85500000>;
diff --git a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev05.dts b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev05.dts
index d481339d..75c09c12 100755
--- a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev05.dts
+++ b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev05.dts
@@ -27,7 +27,7 @@
 
 / {
 	model = "Spreadtrum SP7730G board";
-        sprd,sc-id = <8830 5 0x20000>;
+        qcom,msm-id = <8830 5 0x20000>;
 	chosen {
 		bootargs = "init=/init root=/dev/ram0 rw";
 		linux,initrd-start = <0x85500000>;
diff --git a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev06.dts b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev06.dts
index 1d9f7fbe..5c5b6bd3 100755
--- a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev06.dts
+++ b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev06.dts
@@ -27,7 +27,7 @@
 
 / {
 	model = "Spreadtrum SP7730G board";
-        sprd,sc-id = <8830 6 0x20000>;
+        qcom,msm-id = <8830 6 0x20000>;
 	chosen {
 		bootargs = "init=/init root=/dev/ram0 rw";
 		linux,initrd-start = <0x85500000>;
diff --git a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev07.dts b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev07.dts
index f14b2001..f72fd561 100755
--- a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev07.dts
+++ b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev07.dts
@@ -27,7 +27,7 @@
 
 / {
 	model = "Spreadtrum SP7730G board";
-        sprd,sc-id = <8830 7 0x20000>;
+        qcom,msm-id = <8830 7 0x20000>;
 	chosen {
 		bootargs = "init=/init root=/dev/ram0 rw";
 		linux,initrd-start = <0x85500000>;
diff --git a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev08.dts b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev08.dts
index c0909b14..dfa807bd 100755
--- a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev08.dts
+++ b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev08.dts
@@ -27,7 +27,7 @@
 
 / {
 	model = "Spreadtrum SP7730G board";
-        sprd,sc-id = <8830 8 0x20000>;
+        qcom,msm-id = <8830 8 0x20000>;
 	chosen {
 		bootargs = "init=/init root=/dev/ram0 rw";
 		linux,initrd-start = <0x85500000>;
diff --git a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev09.dts b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev09.dts
index 174c8d9f..63bd1224 100755
--- a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev09.dts
+++ b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev09.dts
@@ -27,7 +27,7 @@
 
 / {
 	model = "Spreadtrum SP7730G board";
-        sprd,sc-id = <8830 9 0x20000>;
+        qcom,msm-id = <8830 9 0x20000>;
 	chosen {
 		bootargs = "init=/init root=/dev/ram0 rw";
 		linux,initrd-start = <0x85500000>;
diff --git a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev10.dts b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev10.dts
index 296f0592..6991ba58 100755
--- a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev10.dts
+++ b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev10.dts
@@ -27,7 +27,7 @@
 
 / {
 	model = "Spreadtrum SP7730G board";
-        sprd,sc-id = <8830 10 0x20000>;
+        qcom,msm-id = <8830 10 0x20000>;
 	chosen {
 		bootargs = "init=/init root=/dev/ram0 rw";
 		linux,initrd-start = <0x85500000>;
diff --git a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev11.dts b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev11.dts
index 979167cb..4974526e 100755
--- a/arch/arm/boot/dts/sprd-scx35_gtel3g_rev11.dts
+++ b/arch/arm/boot/dts/sprd-scx35_gtel3g_rev11.dts
@@ -27,7 +27,7 @@
 
 / {
 	model = "Spreadtrum SP7730G board";
-        sprd,sc-id = <8830 11 0x20000>;
+        qcom,msm-id = <8830 11 0x20000>;
 	chosen {
 		bootargs = "init=/init root=/dev/ram0 rw";
 		linux,initrd-start = <0x85500000>;
-- 
2.27.0

