# /etc/inittab

::sysinit:/bin/mount -a
::sysinit:/bin/loadkmap < /etc/keymap.bmap

::once:/sbin/udevd
::once:/bin/udevadm trigger --type=devices --action=add
::once:/bin/udevadm settle
::respawn:/usr/sbin/pb-discover

# Set up getty on framebuffer console
tty1::respawn:/bin/getty -nl /usr/sbin/petitboot-nc 38400 tty1

# Put a getty on the USB serial port
ttyGS0::respawn:/bin/getty -nl /usr/sbin/petitboot-nc 115200 ttyGS0

# Stuff to do for the 3-finger salute
::ctrlaltdel:/bin/reboot

# Stuff to do before rebooting
::shutdown:/bin/umount -a
