SectionVerb {
        EnableSequence [
                cdev "hw:wm8994aif1"

                # Must reset all input/outputs else the mixer goes into a bad
                # state where things randomly don't work.
                cset "name='Headphone Switch' 0"
                cset "name='Speaker Switch' 0"
                cset "name='IN1L Switch' 0"
                cset "name='IN1R Switch' 0"

                cset "name='DAC1R Mixer AIF1.1 Switch' 1"
                cset "name='DAC1L Mixer AIF1.1 Switch' 1"
                cset "name='DAC1 Switch' 1"

                cset "name='Left Headphone Mux' DAC"
                cset "name='Right Headphone Mux' DAC"
        ]

        Value {
                PlaybackPCM "hw:wm8994aif1,0"
                CapturePCM "hw:wm8994aif1,0"
        }
}

SectionDevice."Speaker" {
        Comment "Speaker"

        EnableSequence [
                cdev "hw:wm8994aif1"

                cset "name='SPKR DAC1 Switch' 1"
                cset "name='SPKL DAC1 Switch' 1"
                cset "name='Speaker Switch' 1"
                cset "name='Speaker Boost Volume' 5"
                cset "name='Speaker Mixer Volume' 5"

                exec "echo enable Speaker"
        ]

        Value {
                PlaybackChannels "2"
        }
}

SectionDevice."SpeakerMic" {
        Comment "Speaker and Microphone"

        EnableSequence [
                cdev "hw:wm8994aif1"

                cset "name='SPKR DAC1 Switch' 1"
                cset "name='SPKL DAC1 Switch' 1"
                cset "name='Speaker Switch' 1"
                cset "name='Speaker Boost Volume' 5"
                cset "name='Speaker Mixer Volume' 5"

                cset "name='MIXINL IN1L Switch' 1"
                cset "name='IN1L PGA IN1LP Switch' 1"
                cset "name='IN1L PGA IN1LN Switch' 1"
                cset "name='AIF1ADCL Source' 0"
                cset "name='AIF1ADCR Source' 0"
                cset "name='AIF1ADC1L Mixer ADC/DMIC Switch' 1"
                cset "name='DAC1L Mixer AIF1.1 Switch' 1"
                cset "name='DAC1R Mixer AIF1.1 Switch' 1"

                cset "name='AIF1ADC1 HPF Switch' 1"

                # Mute the mic by default.
                cset "name='IN1L Switch' 0"

                exec "echo enable Speaker and Microphone"
        ]

        Value {
                PlaybackChannels "2"
        }
}

SectionDevice."Headphone" {
        Comment "Headphone"

        EnableSequence [
                cdev "hw:wm8994aif1"
                cset "name='Headphone Switch' 1"

                exec "echo enable Headphone"
        ]

        Value {
                PlaybackChannels "2"
        }
}

SectionDevice."Headset" {
        Comment "Headset"

        EnableSequence [
                cdev "hw:wm8994aif1"
                cset "name='Headphone Switch' 1"

                cset "name='MIXINR IN1R Switch' 1"
                cset "name='IN1R PGA IN1RN Switch' 1"
                cset "name='IN1R PGA IN1RP Switch' 1"
                cset "name='AIF1ADCL Source' 1"
                cset "name='AIF1ADCR Source' 1"
                cset "name='AIF1ADC1R Mixer ADC/DMIC Switch' 1"
                cset "name='DAC1L Mixer AIF1.1 Switch' 1"
                cset "name='DAC1R Mixer AIF1.1 Switch' 1"

                # Mute the mic by default.
                cset "name='IN1R Switch' 0"

                exec "echo enable Headset"
        ]

        Value {
                PlaybackChannels "2"
        }
}
