# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Xunlong Orange Pi 3"
deviceinfo_manufacturer="Xunlong"
deviceinfo_codename="xunlong-orangepi3"
deviceinfo_year="2019"
deviceinfo_dtb="allwinner/sun50i-h6-orangepi-3"
deviceinfo_arch="aarch64"
deviceinfo_disable_dhcpd="true"

# Device related
deviceinfo_gpu_accelerated="true"
deviceinfo_chassis="embedded"
deviceinfo_keyboard="true"
deviceinfo_external_storage="true"
deviceinfo_screen_width="1920"
deviceinfo_screen_height="1080"
deviceinfo_getty="ttyS0;115200"

# Bootloader related
deviceinfo_flash_method="none"
deviceinfo_sd_embed_firmware="u-boot/orangepi_3/u-boot-sunxi-with-spl.bin:8"
deviceinfo_generate_extlinux_config="true"
deviceinfo_kernel_cmdline="rw console=tty0 console=ttyS0,115200 earlycon no_console_suspend panic=10 consoleblank=0 loglevel=1 PMOS_NO_OUTPUT_REDIRECT"
