From a337472571ea8d154e22325a2c06a8b982716fb0 Mon Sep 17 00:00:00 2001
From: Maxim Karasev <begs@disroot.org>
Date: Sat, 4 Sep 2021 14:56:01 +0300
Subject: [PATCH] arm64: dts: allwinner: orangepi-3: fix ethernet

This patch will apply only over Megi's tree. It's based on a larger
patch from LibreELEC tree.
---
 arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
index adf2134ec1a4..82740a8aef9b 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3.dts
@@ -141,7 +141,7 @@ hdmi_out_con: endpoint {
 &emac {
 	pinctrl-names = "default";
 	pinctrl-0 = <&ext_rgmii_pins>;
-	phy-mode = "rgmii-id";
+	phy-mode = "rgmii-txid";
 	phy-handle = <&ext_rgmii_phy>;
 	/*
 	 * The board uses 2.5V RGMII signalling. Power sequence to enable
@@ -151,8 +151,8 @@ &emac {
 	 */
 	phy-supply = <&reg_aldo2>;
 	phy-io-supply = <&reg_gmac_2v5>;
-	allwinner,rx-delay-ps = <200>;
-	allwinner,tx-delay-ps = <200>;
+	allwinner,rx-delay-ps = <1500>;
+	allwinner,tx-delay-ps = <700>;
 	status = "okay";
 };
 
-- 
2.33.0

