diff --git a/arch/arm64/boot/dts/mediatek/mt8183.dtsi b/arch/arm64/boot/dts/mediatek/mt8183.dtsi
index c5e822b6b77a..cf9b087186e7 100644
--- a/arch/arm64/boot/dts/mediatek/mt8183.dtsi
+++ b/arch/arm64/boot/dts/mediatek/mt8183.dtsi
@@ -739,7 +1016,7 @@ THERMAL_NO_LIMIT
 			/* The tzts1 ~ tzts6 don't need to polling */
 			/* The tzts1 ~ tzts6 don't need to thermal throttle */
 
-			tzts1: tzts1 {
+/*			tzts1: tzts1 {
 				polling-delay-passive = <0>;
 				polling-delay = <0>;
 				thermal-sensors = <&thermal 1>;
@@ -791,7 +1068,7 @@ tztsABB: tztsABB {
 				sustainable-power = <5000>;
 				trips {};
 				cooling-maps {};
-			};
+			}; */
 		};
 
 		pwm0: pwm@1100e000 {
