# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Pine64 PineNote"
deviceinfo_manufacturer="Pine64"
deviceinfo_codename="pine64-pinenote"
deviceinfo_year="2021"
deviceinfo_dtb="rockchip/rk3566-pinenote-v1.2"
deviceinfo_arch="aarch64"
deviceinfo_gpu_accelerated="true"

# Device related
deviceinfo_chassis="tablet"
deviceinfo_keyboard="false"
deviceinfo_external_storage="false"
deviceinfo_screen_width="1404"
deviceinfo_screen_height="1872"
deviceinfo_getty="ttyS2;1500000"

# initfs
deviceinfo_modules_initfs="tps65185-regulator rockchip_ebc drm_kms_helper drm_shmem_helper pvi_waveform"

# Bootloader related
deviceinfo_flash_method="rkdeveloptool"
deviceinfo_flash_sparse="true"

deviceinfo_flash_rk_partition_kernel="cache"
deviceinfo_flash_rk_partition_system="userdata"

deviceinfo_generate_extlinux_config="true"
deviceinfo_kernel_cmdline="earlycon console=tty0 console=ttyS2,1500000n8 PMOS_NO_OUTPUT_REDIRECT vt.default_red=0xFF,0xBC,0x4F,0xB4,0x56,0xBC,0x4F,0x00,0xA1,0xCF,0x84,0xCA,0x8D,0xB4,0x84,0x68 vt.default_grn=0xFF,0x55,0xBA,0xBA,0x4D,0x4D,0xB3,0x00,0xA0,0x8F,0xB3,0xCA,0x88,0x93,0xA4,0x68 vt.default_blu=0xFF,0x58,0x5F,0x58,0xC5,0xBD,0xC5,0x00,0xA8,0xBB,0xAB,0x97,0xBD,0xC7,0xC5,0x68 PMOS_FORCE_PARTITION_RESIZE"
