From be67f67c4ac44b571d1740c1da10669fe6a5c75b Mon Sep 17 00:00:00 2001
From: Robert Mader <robert.mader@collabora.com>
Date: Wed, 1 May 2024 18:12:02 +0200
Subject: [PATCH 1/2] libcamera: simple: Enable softISP for the Pinephone

In theory the PP should be able to use the actual HW ISP, however in
practice this does not work well yet - especially as the driver for the
front camera in Megi differs heavily from the upstream one.

Thus enable the swISP to make both cameras work reliably for now. This
is essentially what Megapixels does as well. If the HW ISP situation
improves, this can be dropped again.

Signed-off-by: Robert Mader <robert.mader@collabora.com>
---
 src/libcamera/pipeline/simple/simple.cpp | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/src/libcamera/pipeline/simple/simple.cpp b/src/libcamera/pipeline/simple/simple.cpp
index e26f438d9..24538649c 100644
--- a/src/libcamera/pipeline/simple/simple.cpp
+++ b/src/libcamera/pipeline/simple/simple.cpp
@@ -264,7 +264,7 @@ static const SimplePipelineInfo supportedDevices[] = {
 	{ "mtk-seninf", { { "mtk-mdp", 3 } }, false },
 	{ "mxc-isi", {}, false },
 	{ "qcom-camss", {}, true },
-	{ "sun6i-csi", {}, false },
+	{ "sun6i-csi", {}, true },
 };
 
 bool isRaw(const StreamConfiguration &cfg)
-- 
2.55.0

