# Archived: Downstream port, only for testing. Use mainline port (asus-x00td)!
# This kernel is mostly used for bringing up new features on mainline, thus unmaintained
# Reference: <https://postmarketos.org/devicepkg>
maintainer=""
pkgname=device-asus-x00td-downstream
pkgdesc="Asus Zenfone Max Pro M1 downstream"
pkgver=4
pkgrel=0
url="postmarketos.org"
arch="aarch64"
license="MIT"
options="!check !archcheck"
depends="linux-asus-x00td-downstream mkbootimg msm-fb-refresher postmarketos-base"
makedepends="devicepkg-dev"
source="deviceinfo kernel-cmdline.conf"

build() {
	devicepkg_build $startdir $pkgname
}

package() {
	devicepkg_package $startdir $pkgname
}

sha512sums="
dba81cd79eb19593fb886918cb2f9595e2b7b656eba4569e646f443c010671d5b48343cc203173036879a6c81c95eb90e02d20f8795c9b5d5f5dfe08740978d9  deviceinfo
4b2ea9d473de336b68db736b2b2ae44e8f952a948c016fbbceb205512f73548b85cb00a488f600f1346e92dc839d2ee2419fbd5bf56f9cba9df843419b69ec74  kernel-cmdline.conf
"
