From 073fd00aa6e0874406366de291a07b79f22c8758 Mon Sep 17 00:00:00 2001
From: Jun Nie <jun.nie@linaro.org>
Date: Wed, 1 Oct 2025 21:59:13 +0800
Subject: [PATCH 05/12] drm/msm/dsi: support DSC configurations with
 slice_per_pkt > 1

Some panels support multiple slice to be sent in a single DSC packet. And
this feature is a must for specific panels, such as JDI LPM026M648C. Add a
dsc_slice_per_pkt member into struct mipi_dsi_device and support the
feature in msm mdss driver.

Co-developed-by: Jonathan Marek <jonathan@marek.ca>
Signed-off-by: Jonathan Marek <jonathan@marek.ca>
Signed-off-by: Jun Nie <jun.nie@linaro.org>
Signed-off-by: Junjie Cao <caojunjie650@gmail.com>
---
 drivers/gpu/drm/msm/dsi/dsi_host.c | 25 ++++++++++---------------
 include/drm/drm_mipi_dsi.h         |  2 ++
 2 files changed, 12 insertions(+), 15 deletions(-)

diff --git a/drivers/gpu/drm/msm/dsi/dsi_host.c b/drivers/gpu/drm/msm/dsi/dsi_host.c
index db6da99375a1..519410ec5197 100644
--- a/drivers/gpu/drm/msm/dsi/dsi_host.c
+++ b/drivers/gpu/drm/msm/dsi/dsi_host.c
@@ -166,6 +166,7 @@ struct msm_dsi_host {
 
 	struct drm_display_mode *mode;
 	struct drm_dsc_config *dsc;
+	unsigned int dsc_slice_per_pkt;
 
 	/* connected device info */
 	unsigned int channel;
@@ -927,17 +928,10 @@ static void dsi_update_dsc_timing(struct msm_dsi_host *msm_host, bool is_cmd_mod
 	slice_per_intf = dsc->slice_count;
 
 	total_bytes_per_intf = dsc->slice_chunk_size * slice_per_intf;
-	bytes_per_pkt = dsc->slice_chunk_size; /* * slice_per_pkt; */
+	bytes_per_pkt = dsc->slice_chunk_size * msm_host->dsc_slice_per_pkt;
 
 	eol_byte_num = total_bytes_per_intf % 3;
-
-	/*
-	 * Typically, pkt_per_line = slice_per_intf * slice_per_pkt.
-	 *
-	 * Since the current driver only supports slice_per_pkt = 1,
-	 * pkt_per_line will be equal to slice per intf for now.
-	 */
-	pkt_per_line = slice_per_intf;
+	pkt_per_line = slice_per_intf / msm_host->dsc_slice_per_pkt;
 
 	if (is_cmd_mode) /* packet data type */
 		reg = DSI_COMMAND_COMPRESSION_MODE_CTRL_STREAM0_DATATYPE(MIPI_DSI_DCS_LONG_WRITE);
@@ -1088,12 +1082,8 @@ static void dsi_timing_setup(struct msm_dsi_host *msm_host, bool is_bonded_dsi)
 		else
 			/*
 			 * When DSC is enabled, WC = slice_chunk_size * slice_per_pkt + 1.
-			 * Currently, the driver only supports default value of slice_per_pkt = 1
-			 *
-			 * TODO: Expand mipi_dsi_device struct to hold slice_per_pkt info
-			 *       and adjust DSC math to account for slice_per_pkt.
 			 */
-			wc = msm_host->dsc->slice_chunk_size + 1;
+			wc = msm_host->dsc->slice_chunk_size * msm_host->dsc_slice_per_pkt + 1;
 
 		dsi_write(msm_host, REG_DSI_CMD_MDP_STREAM0_CTRL,
 			DSI_CMD_MDP_STREAM0_CTRL_WORD_COUNT(wc) |
@@ -1702,8 +1692,13 @@ static int dsi_host_attach(struct mipi_dsi_host *host,
 	msm_host->lanes = dsi->lanes;
 	msm_host->format = dsi->format;
 	msm_host->mode_flags = dsi->mode_flags;
-	if (dsi->dsc)
+	if (dsi->dsc) {
 		msm_host->dsc = dsi->dsc;
+		msm_host->dsc_slice_per_pkt = dsi->dsc_slice_per_pkt;
+		/* for backwards compatibility, assume 1 if not set */
+		if (!msm_host->dsc_slice_per_pkt)
+			msm_host->dsc_slice_per_pkt = 1;
+	}
 
 	ret = dsi_dev_attach(msm_host->pdev);
 	if (ret)
diff --git a/include/drm/drm_mipi_dsi.h b/include/drm/drm_mipi_dsi.h
index 3aba7b380c8d..2ddec7931bd0 100644
--- a/include/drm/drm_mipi_dsi.h
+++ b/include/drm/drm_mipi_dsi.h
@@ -180,6 +180,7 @@ struct mipi_dsi_device_info {
  * be set to the real limits of the hardware, zero is only accepted for
  * legacy drivers
  * @dsc: panel/bridge DSC pps payload to be sent
+ * @dsc_slice_per_pkt: number of DSC slices to be sent as in a single packet
  */
 struct mipi_dsi_device {
 	struct mipi_dsi_host *host;
@@ -194,6 +195,7 @@ struct mipi_dsi_device {
 	unsigned long hs_rate;
 	unsigned long lp_rate;
 	struct drm_dsc_config *dsc;
+	unsigned int dsc_slice_per_pkt;
 };
 
 /**
-- 
2.52.0

