diff --git a/arch/arm64/boot/dts/qcom/sm8150-xiaomi-nabu.dts b/arch/arm64/boot/dts/qcom/sm8150-xiaomi-nabu.dts
index dfebc7f3e70c..b7845863eaa1 100644
--- a/arch/arm64/boot/dts/qcom/sm8150-xiaomi-nabu.dts
+++ b/arch/arm64/boot/dts/qcom/sm8150-xiaomi-nabu.dts
@@ -198,7 +198,7 @@ event-hall-sensor {
 			linux,code = <SW_LID>;
 			debounce-interval = <15>;
 			linux,can-disable;
-			wakeup-source;
+			// wakeup-source;
 		};
 	};
 };
