# Archived: Downstream port, only for testing. Use mainline port!
# Reference: <https://postmarketos.org/devicepkg>
maintainer=""
pkgname=device-sony-tulip-downstream
pkgdesc="Sony Xperia M4 Aqua"
pkgver=4
pkgrel=0
url="https://postmarketos.org"
license="MIT"
arch="aarch64"
options="!check !archcheck"
depends="postmarketos-base linux-sony-tulip mkbootimg"
makedepends="devicepkg-dev"
source="deviceinfo kernel-cmdline.conf"

build() {
	devicepkg_build $startdir $pkgname
}

package() {
	devicepkg_package $startdir $pkgname
}


sha512sums="
8beb8a48a081649037472e29849cd9e7977b82ef60e80189df4e4c590bc85679e4b8f62ca70dff616896d911de20605ee3358d6613a4238a2c4183e3ad9659b2  deviceinfo
90bd491c0f60806d9d7ebecb996de9067707d9a32d4ec2ce4f9e17330a677d03c43d4d989712e5dea7888f5301a959e7344ef079b644bad350c0fbbbe6c61d5d  kernel-cmdline.conf
"
