# Archived: unmaintained port, only for testing. Use generic/mainline port (qcom-msm8953)
maintainer=""
pkgname=firmware-xiaomi-tissot
pkgver=2
pkgrel=2
pkgdesc="Firmware files for Xiaomi Mi A1"
url="https://gitlab.com/jiaxyga/firmware-xiaomi-tissot"
arch="aarch64"
license="proprietary"
options="!strip !check !archcheck !spdx !tracedeps pmb:cross-native"

_commit="bf686895224cae33c2130932b4a5914fea415287"

source="$pkgname-$_commit.tar.gz::$url/-/archive/$_commit/$pkgname-$_commit.tar.gz"
builddir="$srcdir/$pkgname-$_commit/lib/firmware/postmarketos"
_fwdir="/lib/firmware/qcom/msm8953/xiaomi/tissot"

package() {
	# GPU firmwares
	install -Dm644 a506_zap.b02 -t "$pkgdir/$_fwdir"
	install -Dm644 a506_zap.mdt -t "$pkgdir/$_fwdir"
}

sha512sums="
e82c953fd1a1a665bcfcfc4eaab95fe8a017f1804e4bc66f6449cfeb21137f2ebcc0f8abab9ef9975c438d9836d68974b417bbe58c128b06cec605abecfad008  firmware-xiaomi-tissot-bf686895224cae33c2130932b4a5914fea415287.tar.gz
"
