# Archived: Downstream port, only for testing. Use mainline port!
# Reference: <https://postmarketos.org/devicepkg>
maintainer="Luca Weiss <luca@lucaweiss.eu>"
pkgname=device-huawei-sturgeon-downstream
pkgdesc="Huawei Watch"
pkgver=4
pkgrel=0
url="https://postmarketos.org"
license="MIT"
arch="armv7"
options="!check !archcheck"
depends="
	firmware-huawei-sturgeon-adsp
	firmware-huawei-sturgeon-wifi
	linux-huawei-sturgeon
	mkbootimg
	msm-fb-refresher
	postmarketos-base
"
makedepends="devicepkg-dev"
source="
	deviceinfo
	kernel-cmdline.conf
	networkmanager.conf
"

build() {
	devicepkg_build $startdir $pkgname
}

package() {
	devicepkg_package $startdir $pkgname
}

sha512sums="
728b39211adf1f8fadadfc250f8e5c19bde5f392199eabc6a09698369472b3b599ae37980581f36ea23cbc48496f569259a6b10df58a77488ae680b847546486  deviceinfo
15307969581076bbd48997d947fc74a79d331de83d13a6b327c6f0db6f9b35f91a47486838d83f6d21634a267d5ac7d8d7c0e9a08b0198be240a519973f8618a  kernel-cmdline.conf
a19923f30ac1d328a85ab1162e44442da28dd1ae45529fb73e21d8004594487f61c8f5372e5bbaadfefd27fe27c8a22ce430b81891ac1965e5704bbfec108b82  networkmanager.conf
"
