From fba887bbded01ab5ce2293f6e624e833759559cd Mon Sep 17 00:00:00 2001
From: Martijn Braam <martijn@brixit.nl>
Date: Tue, 20 Oct 2020 14:44:51 +0200
Subject: [PATCH] dts: pinetab: make audio routing consistent with pinephone

---
 arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts | 10 +++++-----
 1 file changed, 5 insertions(+), 5 deletions(-)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts
index e30034a1553b..b2a3c0f97ce1 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts
@@ -494,13 +494,13 @@ &sound {
 				    "Headphone", "Headphone Jack",
 				    "Speaker", "Internal Speaker";
 	simple-audio-card,routing =
-			"Left DAC", "DACL",
-			"Right DAC", "DACR",
-			"Speaker Amp INL", "LINEOUT",
-			"Speaker Amp INR", "LINEOUT",
+			"Headphone Jack", "HP",
 			"Internal Speaker", "Speaker Amp OUTL",
 			"Internal Speaker", "Speaker Amp OUTR",
-			"Headphone Jack", "HP",
+			"Speaker Amp INL", "LINEOUT",
+			"Speaker Amp INR", "LINEOUT",
+			"Left DAC", "DACL",
+			"Right DAC", "DACR",
 			"ADCL", "Left ADC",
 			"ADCR", "Right ADC",
 			"Internal Microphone Left", "MBIAS",
-- 
2.52.0

