# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Qualcomm SDM845 device"
deviceinfo_manufacturer="Qualcomm"
deviceinfo_codename="qualcomm-sdm845"
deviceinfo_year="2023"
deviceinfo_arch="aarch64"

# Device related
deviceinfo_drm="true"
deviceinfo_external_storage="true"

# Bootloader related
deviceinfo_flash_method="fastboot-bootpart"
# Where to flash boot.img, or in our case where to flash the pmOS boot partition.
# This is a bit confusing.
deviceinfo_flash_fastboot_partition_kernel="system"
deviceinfo_getty="ttyMSM0;115200"
deviceinfo_boot_filesystem="fat32"

# Look ma! no hands!
# u-boot picks the right DTB for us, no need to specify it in systemd-boot.
# deviceinfo_dtb=""
deviceinfo_initfs_compression="zstd:fast"

# Required for devices using UFS as storage (instead of e.g. eMMC)
deviceinfo_rootfs_image_sector_size="4096"

