# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Epson Moverio BT-200"
deviceinfo_manufacturer="Epson"
deviceinfo_codename="epson-embt2ws"
deviceinfo_year="2014"
deviceinfo_arch="armv7"
deviceinfo_dtb="omap4-epson-embt2ws"
deviceinfo_generate_extlinux_config="true"
# Device related
# chassis = touchpad with buttons + glasses
deviceinfo_chassis="embedded"
deviceinfo_external_storage="true"

# Bootloader related
deviceinfo_boot_filesystem="fat32"
deviceinfo_getty="ttyS2;115200"
deviceinfo_no_framebuffer="true"

# for using the sdboot.scr mechanism to chainload stuff from internal u-boot,
# GPT does not work, if a standalone u-boot install is used, GPT is ok.
deviceinfo_partition_type="msdos"

deviceinfo_sd_embed_firmware_step_size="512"
deviceinfo_sd_embed_firmware="u-boot/epson-embt2ws/MLO:256,u-boot/epson-embt2ws/u-boot.img:512"
