# Archived: Downstream port, only for testing. Use mainline port!
# Reference: <https://postmarketos.org/devicepkg>
maintainer=""
pkgname=device-motorola-falcon-downstream
pkgdesc="Moto G (2013) (Downstream)"
pkgver=4
pkgrel=0
url="https://postmarketos.org"
license="MIT"
arch="armv7"
options="!check !archcheck"
depends="
	firmware-motorola-falcon
	linux-motorola-falcon-downstream
	mkbootimg
	msm-fb-refresher
	postmarketos-base
	"
makedepends="devicepkg-dev"
source="
	deviceinfo
	kernel-cmdline.conf
	"

build() {
	devicepkg_build $startdir $pkgname
}

package() {
	devicepkg_package $startdir $pkgname
}

sha512sums="
c4e1d926710feffc378d26544835a18f5d0bf6405de29bbefe15e4c0fd45878b35d7caa55aca0e1c5a9faf489c12464a4d9cf503cad9a0dd515cb81f7447e44c  deviceinfo
041616fe111ac217376660feb5a9e57550f585f59033e84d4550679ac150cdb827da17d9cdb65580b23e11170ed751f8e1d77c2830a16bb9e5aadea9a83f0320  kernel-cmdline.conf
"
