# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Google Oak Chromebook"
deviceinfo_manufacturer="Google"
deviceinfo_codename="google-oak"
deviceinfo_year="2017"
deviceinfo_dtb="mediatek/mt8173-elm*"
deviceinfo_arch="aarch64"

# Device related
# chassis does not make sense here, will probably be removed (pmb#2255)
deviceinfo_chassis="convertible"
deviceinfo_external_storage="true"
deviceinfo_screen_width="1366"
deviceinfo_screen_height="768"
deviceinfo_disable_dhcpd="true"
deviceinfo_create_initfs_extra="true"

# Bootloader related
deviceinfo_cgpt_kpart="/boot/vmlinuz.kpart"
deviceinfo_cgpt_kpart_start="8192"
deviceinfo_cgpt_kpart_size="65536"
# We are supposed to use "oak" board here, but lazor dts does
# not include oak compatible which results in loading a wrong
# dtb. "mt8173" board may result in including dtbs that are for
# mt8173 but not related to Chrome OS devices which would increase
# image size. This doesn't happen for us because we provide only
# dtbs from deviceinfo_dtb variable and nothing more, so use "mt8173"
# board here.
deviceinfo_depthcharge_board="mt8173"
deviceinfo_depthcharge_compression="lzma"
deviceinfo_generate_depthcharge_image="true"
