# Archived: unmaintained port, only for testing. Use generic/mainline port (qcom-msm8953)
# Reference: <https://postmarketos.org/devicepkg>
maintainer=""
pkgname=device-xiaomi-vince
pkgdesc="Xiaomi Redmi 5 Plus"
pkgver=18
pkgrel=0
url="https://postmarketos.org"
license="MIT"
arch="aarch64"
options="!check !archcheck"
depends="
	firmware-qcom-adreno-a530
	firmware-xiaomi-vince
	linux-postmarketos-qcom-msm8953
	lk2nd-msm8953
	mkbootimg
	msm-firmware-loader
	postmarketos-base
	soc-qcom-msm8953
	soc-qcom-msm8953-modem
"
makedepends="devicepkg-dev"
source="
	deviceinfo
	modules-initfs
"

build() {
	devicepkg_build $startdir $pkgname
}

package() {
	devicepkg_package $startdir $pkgname
}

sha512sums="
51940546488682493507f688c0fc97384d1c6a37bd78d940adffc7cfcf06a6b44a4287312bf11e645d2d5c99dfa9118ac968c984723e5c49c9d16e5b0550bc0c  deviceinfo
69cfc8db6ea497576085e1b5861c766b5c6cfbd493e4d66aa0bfa29a0e80eeaeb8a465c4841c6a7959796f5a2325e621d60f2c35ccb0741d7934ab310abe807f  modules-initfs
"
