# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="Samsung Galaxy Note 3"
deviceinfo_manufacturer="Samsung"
deviceinfo_codename="samsung-hlte"
deviceinfo_year="2013"
deviceinfo_dtb="qcom-msm8974-samsung-hlte"
deviceinfo_append_dtb="true"
deviceinfo_modules_initfs="pm8941_pwrkey rmi_core rmi_i2c panel-samsung-s6e3fa0"
deviceinfo_arch="armv7"

# Device related
deviceinfo_chassis="handset"
deviceinfo_keyboard="false"
deviceinfo_external_storage="true"
deviceinfo_screen_width="1080"
deviceinfo_screen_height="1920"
deviceinfo_getty="ttyMSM0;115200"
deviceinfo_gpu_accelerated="true"

# Bootloader related
deviceinfo_flash_method="heimdall-bootimg"
deviceinfo_kernel_cmdline="console=ttyMSM0,115200,n8 msm.vram=192m msm.allow_vram_carveout=1 PMOS_NO_OUTPUT_REDIRECT"
deviceinfo_generate_bootimg="true"
deviceinfo_bootimg_qcdt="false"
deviceinfo_bootimg_append_seandroidenforce="true"
deviceinfo_flash_offset_base="0x00000000"
deviceinfo_flash_offset_kernel="0x00008000"
deviceinfo_flash_offset_ramdisk="0x02900000"
deviceinfo_flash_offset_second="0x00f00000"
deviceinfo_flash_offset_tags="0x02700000"
deviceinfo_flash_pagesize="2048"
deviceinfo_flash_heimdall_partition_kernel="BOOT"

# Samsung Electronics Co., Ltd
deviceinfo_usb_idVendor="0x04e8"
# Galaxy (MTP)
deviceinfo_usb_idProduct="0x6860"
