# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="Mobvoi Ticwatch C2"
deviceinfo_manufacturer="Mobvoi"
deviceinfo_codename="mobvoi-skipjack"
deviceinfo_year="2018"
deviceinfo_arch="armv7"

# Device related
deviceinfo_chassis="watch"
deviceinfo_keyboard="false"
deviceinfo_external_storage="false"
deviceinfo_screen_width="360"
deviceinfo_screen_height="360"

# Bootloader related
deviceinfo_flash_method="fastboot"
deviceinfo_flash_sparse="true"
deviceinfo_kernel_cmdline="androidboot.hardware=skipjack msm_rtb.filter=0x237 ehci-hcd.park=3 lpm_levels.sleep_disabled=1 androidboot.selinux=permissive buildvariant=eng"
deviceinfo_generate_bootimg="true"
deviceinfo_bootimg_qcdt="false"
deviceinfo_bootimg_mtk_mkimage="false"
deviceinfo_bootimg_dtb_second="false"
deviceinfo_flash_pagesize="2048"
deviceinfo_flash_offset_base="0x80100000"
deviceinfo_flash_offset_kernel="0x00008000"
deviceinfo_flash_offset_ramdisk="0x02000000"
deviceinfo_flash_offset_second="0x00f00000"
deviceinfo_flash_offset_tags="0x01e00000"
