From 4ae995b8dbef63a3253c40aa08e09b16c3008425 Mon Sep 17 00:00:00 2001
From: JuniorJPDJ <git@juniorjpdj.pl>
Date: Sun, 28 Mar 2021 03:05:32 +0200
Subject: [PATCH] configs: add goclever-gcta741l

---
 configs/goclever-gcta741l_defconfig | 27 +++++++++++++++++++++++++++
 1 file changed, 27 insertions(+)
 create mode 100644 configs/goclever-gcta741l_defconfig

diff --git a/configs/goclever-gcta741l_defconfig b/configs/goclever-gcta741l_defconfig
new file mode 100644
index 0000000000..0c23d3ab04
--- /dev/null
+++ b/configs/goclever-gcta741l_defconfig
@@ -0,0 +1,27 @@
+CONFIG_ARM=y
+CONFIG_ARCH_SUNXI=y
+CONFIG_SPL=y
+CONFIG_MACH_SUN6I=y
+CONFIG_DRAM_CLK=360
+CONFIG_DRAM_ZQ=251
+CONFIG_MMC0_CD_PIN="PA8"
+CONFIG_USB0_VBUS_PIN="AXP0-VBUS-ENABLE"
+CONFIG_USB0_VBUS_DET="AXP0-VBUS-DETECT"
+CONFIG_USB0_ID_DET="PA15"
+CONFIG_AXP_GPIO=y
+CONFIG_VIDEO_LCD_MODE="x:800,y:480,depth:18,pclk_khz:33000,le:14,ri:240,up:3,lo:35,hs:30,vs:13,sync:3,vmode:0"
+# le=-14,up=-3
+CONFIG_VIDEO_LCD_DCLK_PHASE=0
+CONFIG_VIDEO_LCD_BL_EN="PA25"
+CONFIG_VIDEO_LCD_BL_PWM="PH13"
+CONFIG_NR_DRAM_BANKS=1
+CONFIG_SPL_TEXT_BASE=0x60
+# CONFIG_SYS_MALLOC_CLEAR_ON_INIT is not set
+CONFIG_DEFAULT_DEVICE_TREE="sun6i-a31s-goclever-gcta741l"
+CONFIG_AXP_DLDO1_VOLT=3300
+CONFIG_USB_EHCI_HCD=y
+CONFIG_USB_OHCI_HCD=y
+CONFIG_USB_MUSB_HOST=y
+CONFIG_USB_KEYBOARD=y
+CONFIG_USB_STORAGE=y
+CONFIG_SYS_USB_EVENT_POLL_VIA_INT_QUEUE=y
-- 
2.31.0

