# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell
# scripts.

deviceinfo_format_version="0"
deviceinfo_name="DongshanPi NeZha STU"
deviceinfo_manufacturer="DongshanPi"
deviceinfo_codename="dongshanpi-nezhastu"
deviceinfo_year="2022"
deviceinfo_dtb="allwinner/sun20i-d1-dongshan-nezha-stu"
deviceinfo_arch="riscv64"

# Device related
deviceinfo_gpu_accelerated="false"
deviceinfo_chassis="embedded"
deviceinfo_keyboard="true"
deviceinfo_external_storage="true"
deviceinfo_screen_width="1920"
deviceinfo_screen_height="1080"
deviceinfo_getty="ttyS0;115200"

# Bootloader related
deviceinfo_flash_method="none"
deviceinfo_sd_embed_firmware="u-boot/dongshan_nezha_stu/u-boot-sunxi-with-spl.bin:8"
deviceinfo_boot_part_start="8192"
deviceinfo_kernel_cmdline="console=ttyS0,115200 no_console_suspend panic=10 PMOS_NO_OUTPUT_REDIRECT"
deviceinfo_generate_grub_config="true"
