#!/usr/sbin/nft -f

table inet filter {
	chain input {

		# Allow DHCP server on usb*
		iifname "usb*" udp dport bootps accept comment "accept incoming DHCP on usb*"

		# Allow DHCP server on wlan* for hotspot
		iifname "wlan*" udp dport bootps accept comment "accept incoming DHCP on wlan*"
	}
}
