pkgname=firmware-xiaomi-daisy
pkgver=1
pkgrel=1
pkgdesc="Firmware files for Xiaomi Mi A2 Lite"
url="https://postmarketos.org"
arch="aarch64"
license="proprietary"
depends="wcnss-wlan"
_repository="firmware-xiaomi-daisy"
_commit="9ae200b57743088f83a6f2b02a6b7ce4596a77d6"
source="$pkgname-$_commit.tar.gz::https://github.com/alikates/firmware-xiaomi-daisy/archive/$_commit.tar.gz"
options="!strip !check !archcheck !spdx !tracedeps pmb:cross-native"
builddir="$srcdir/firmware-xiaomi-daisy-$_commit"

_fwdir="/lib/firmware/postmarketos"

package() {
	echo $source

	# Modem firmware
	install -Dm0644 modem/mba.mbn -t "$pkgdir/$_fwdir"
	install -Dm0644 modem/modem.* -t "$pkgdir/$_fwdir"

	# ADSP firmware
	install -Dm0644 adsp/adsp.* -t "$pkgdir/$_fwdir"

	# GPU and video acceleration firmwares
	install -Dm0644 gpu/a5* -t "$pkgdir/$_fwdir"
	install -Dm0644 gpu/venus.* -t "$pkgdir/$_fwdir"

	# Wifi/BT firmware
	install -Dm0644 wcnss/WCNSS_qcom_wlan_nv.bin -t "$pkgdir/$_fwdir"/wlan/prima
	install -Dm0644 wcnss/wcnss.* -t "$pkgdir/$_fwdir"
}

sha512sums="
0778b0c4a7e836c9e0cef842dda2fd9d5eba4693cd875a605413267690d48d9b7ea86b1ece0471e55e5c49d1b3645bee1aa735ba164d0120bdfc94ffffa7e16b  firmware-xiaomi-daisy-9ae200b57743088f83a6f2b02a6b7ce4596a77d6.tar.gz
"
