diff --git a/configs/pinebook-pro-rk3399_defconfig b/configs/pinebook-pro-rk3399_defconfig
index 21eecf477c..733463556a 100644
--- a/configs/pinebook-pro-rk3399_defconfig
+++ b/configs/pinebook-pro-rk3399_defconfig
@@ -61,6 +61,8 @@ CONFIG_RAM_RK3399_LPDDR4=y
 CONFIG_DM_RESET=y
 CONFIG_BAUDRATE=1500000
 CONFIG_DEBUG_UART_SHIFT=2
+CONFIG_USE_PREBOOT=y
+CONFIG_PREBOOT="usb start"
 CONFIG_ROCKCHIP_SPI=y
 CONFIG_SYSRESET=y
 CONFIG_USB=y
@@ -68,8 +70,11 @@ CONFIG_USB_XHCI_HCD=y
 CONFIG_USB_XHCI_DWC3=y
 CONFIG_USB_EHCI_HCD=y
 CONFIG_USB_EHCI_GENERIC=y
+CONFIG_USB_OHCI_HCD=y
+CONFIG_USB_OHCI_GENERIC=y
 CONFIG_USB_DWC3=y
 CONFIG_ROCKCHIP_USB2_PHY=y
+CONFIG_DM_KEYBOARD=y
 CONFIG_USB_KEYBOARD=y
 CONFIG_USB_HOST_ETHER=y
 CONFIG_USB_ETHER_ASIX=y
diff --git a/include/configs/pinebook-pro-rk3399.h b/include/configs/pinebook-pro-rk3399.h
index 4bc8802d11..d910830582 100644
--- a/include/configs/pinebook-pro-rk3399.h
+++ b/include/configs/pinebook-pro-rk3399.h
@@ -25,4 +25,7 @@
 
 #define SDRAM_BANK_SIZE			(2UL << 30)
 
+#define CONFIG_USB_OHCI_NEW
+#define CONFIG_SYS_USB_OHCI_MAX_ROOT_PORTS     2
+
 #endif
