From b25dcb4f2ece56b03a09680ba933f8788bc64864 Mon Sep 17 00:00:00 2001
From: Wolfgang Wiedmeyer <wolfgit@wiedmeyer.de>
Date: Mon, 26 Sep 2016 23:33:05 +0200
Subject: [PATCH 06/11] mfd: max77693: Add defines for charger current control

This prepares for an updated regulator and charger driver. The defines
are needed to set the maximum input current and the fast charge
current.

Signed-off-by: Wolfgang Wiedmeyer <wolfgit@wiedmeyer.de>
GNUtoo@cyberdimension.org: small fix
Signed-off-by: Denis 'GNUtoo' Carikli <GNUtoo@cyberdimension.org>
---
 include/linux/mfd/max77693-private.h | 7 +++++++
 1 file changed, 7 insertions(+)

diff --git a/include/linux/mfd/max77693-private.h b/include/linux/mfd/max77693-private.h
index 311f7d3d2323..f6df8bafe996 100644
--- a/include/linux/mfd/max77693-private.h
+++ b/include/linux/mfd/max77693-private.h
@@ -217,6 +217,9 @@ enum max77693_charger_battery_state {
 #define CHG_CNFG_01_CHGRSTRT_MASK	(0x3 << CHG_CNFG_01_CHGRSTRT_SHIFT)
 #define CHG_CNFG_01_PQEN_MAKS		BIT(CHG_CNFG_01_PQEN_SHIFT)
 
+/* MAX77693_CHG_REG_CHG_CNFG_02 register */
+#define CHG_CNFG_02_CC_MASK		0x3F
+
 /* MAX77693_CHG_REG_CHG_CNFG_03 register */
 #define CHG_CNFG_03_TOITH_SHIFT		0
 #define CHG_CNFG_03_TOTIME_SHIFT	3
@@ -245,6 +248,10 @@ enum max77693_charger_battery_state {
 
 /* MAX77693 CHG_CNFG_09 Register */
 #define CHG_CNFG_09_CHGIN_ILIM_MASK	0x7F
+#define CHG_CNFG_09_CHGIN_ILIM_500_MAX	500000
+#define CHG_CNFG_09_CHGIN_ILIM_500_MIN	470000
+#define CHG_CNFG_09_CHGIN_ILIM_0_MAX	60000
+#define CHG_CNFG_09_CHGIN_ILIM_0_MIN	0
 
 /* MAX77693 CHG_CTRL Register */
 #define SAFEOUT_CTRL_SAFEOUT1_MASK	0x3
-- 
2.38.1

