# Reference: <https://postmarketos.org/devicepkg>
pkgname=device-fairphone-fp2
pkgdesc="Fairphone 2"
pkgver=7
pkgrel=0
url="https://postmarketos.org"
license="MIT"
arch="armv7"
options="!check !archcheck"
depends="
	mkbootimg
	postmarketos-base
	swclock-offset
	"
makedepends="devicepkg-dev"
source="deviceinfo
	FP2.conf
	hifi
	phoc.ini
	30-gpu-firmware.files
"
subpackages="
	$pkgname-kernel-downstream:kernel_downstream
	$pkgname-kernel-mainline:kernel_mainline
	$pkgname-nonfree-firmware:nonfree_firmware
	$pkgname-downstream-firmware:downstream_firmware
	$pkgname-mainline-firmware:mainline_firmware
	$pkgname-alsa
	$pkgname-phosh
"

build() {
	devicepkg_build $startdir $pkgname
}

package() {
	devicepkg_package $startdir $pkgname
}

kernel_downstream() {
	pkgdesc="Downstream kernel"
	depends="linux-fairphone-fp2"
	devicepkg_subpackage_kernel $startdir $pkgname $subpkgname
}

kernel_mainline() {
	pkgdesc="Close to mainline kernel"
	depends="linux-postmarketos-qcom-msm8974 mesa-egl"
	devicepkg_subpackage_kernel $startdir $pkgname $subpkgname
}

nonfree_firmware() {
	pkgdesc="Firmware for WiFi, Audio, etc."
	depends="firmware-fairphone-fp2-adsp firmware-fairphone-fp2-modem firmware-fairphone-fp2-wcnss"
	mkdir "$subpkgdir"
}

downstream_firmware() {
	pkgdesc="Firmware support packages for downstream kernel"
	depends="$pkgname-alsa adsp-audio msm-modem-downstream wcnss-wlan"
	install_if="$pkgname-kernel-downstream $pkgname-nonfree-firmware"
	mkdir "$subpkgdir"
}

mainline_firmware() {
	pkgdesc="Firmware support packages for mainline kernel"
	depends="msm-modem msm-modem-uim-selection firmware-qcom-adreno-a330"
	install_if="$pkgname-kernel-mainline $pkgname-nonfree-firmware"
	mkdir "$subpkgdir"

	install -Dm644 "$srcdir/30-gpu-firmware.files" \
		"$subpkgdir/etc/postmarketos-mkinitfs/files/30-gpu-firmware.files"
}

alsa() {
	pkgdesc="Audio configuration files"

	mkdir -p "$subpkgdir"/usr/share/alsa/ucm/FP2
	install -Dm644 "$srcdir"/FP2.conf "$subpkgdir"/usr/share/alsa/ucm/FP2/
	install -Dm644 "$srcdir"/hifi "$subpkgdir"/usr/share/alsa/ucm/FP2/
}

phosh() {
	install_if="$pkgname postmarketos-ui-phosh"
	install -Dm644 "$srcdir"/phoc.ini \
		"$subpkgdir"/etc/phosh/phoc.ini
}

sha512sums="
1327db1026b118ec9f5f74e637e4d7d60763836e6481b0f379be83de2980b7a1c9aed6e0f0dfbd44340a1efd1331e6b21cbac8a968fdf04e7188a990698f9520  deviceinfo
55360b1ba4ddadea341c9edb13c32ba5f19aabf75ab28602f30cfb79b9df8834f115ef979c70569f23ec1293b1fcd408baf320d87803293ce7106bdc73a26c9f  FP2.conf
b834461c6866bb0c473dd089dd5da641dd42a00f610aad6503117aa50fe6e200db9ad0a264bb609f12350d59faee1f772907bacd75439f702ea7d52f6f85e2b1  hifi
cef2fd633cddbcf4ac9b4d2fa6bf3a1e3e8d810a2ea8050767fe649d289db753662821d5e41e2c8d20fb9c765c1babcb6a4d95e4c9345f5ea32d1b1d2b1e5126  phoc.ini
bbe6d6f530a9fa1934dd065dd4f6da48450e2115e4656b219d7f3aebc8b6a2775c02a2e5ffb5790950bb8183fca4677fbeaf9d8a267089c9f0d08461fc8ed45d  30-gpu-firmware.files
"
