From 873c0534790f2f367c5a1851d16c37c3368bcd7f Mon Sep 17 00:00:00 2001
From: Hsin-Yi Wang <hsinyi@chromium.org>
Date: Mon, 13 Dec 2021 15:23:53 +0800
Subject: [PATCH 3/5] arm64: dts: mt8183: Add kukui-jacuzzi-makomo board

Makomo is known as Lenovo 100e Gen 2.

Signed-off-by: Hsin-Yi Wang <hsinyi@chromium.org>
---
 arch/arm64/boot/dts/mediatek/Makefile         |  2 ++
 .../mt8183-kukui-jacuzzi-makomo-sku0.dts      | 24 +++++++++++++++++++
 .../mt8183-kukui-jacuzzi-makomo-sku1.dts      | 24 +++++++++++++++++++
 3 files changed, 50 insertions(+)
 create mode 100644 arch/arm64/boot/dts/mediatek/mt8183-kukui-jacuzzi-makomo-sku0.dts
 create mode 100644 arch/arm64/boot/dts/mediatek/mt8183-kukui-jacuzzi-makomo-sku1.dts

diff --git a/arch/arm64/boot/dts/mediatek/Makefile b/arch/arm64/boot/dts/mediatek/Makefile
index cb8d563d079f..57b33de22981 100644
--- a/arch/arm64/boot/dts/mediatek/Makefile
+++ b/arch/arm64/boot/dts/mediatek/Makefile
@@ -26,6 +26,8 @@ dtb-$(CONFIG_ARCH_MEDIATEK) += mt8183-kukui-jacuzzi-fennel14-sku2.dtb
 dtb-$(CONFIG_ARCH_MEDIATEK) += mt8183-kukui-jacuzzi-juniper-sku16.dtb
 dtb-$(CONFIG_ARCH_MEDIATEK) += mt8183-kukui-jacuzzi-kappa.dtb
 dtb-$(CONFIG_ARCH_MEDIATEK) += mt8183-kukui-jacuzzi-kenzo.dtb
+dtb-$(CONFIG_ARCH_MEDIATEK) += mt8183-kukui-jacuzzi-makomo-sku0.dtb
+dtb-$(CONFIG_ARCH_MEDIATEK) += mt8183-kukui-jacuzzi-makomo-sku1.dtb
 dtb-$(CONFIG_ARCH_MEDIATEK) += mt8183-kukui-jacuzzi-willow-sku0.dtb
 dtb-$(CONFIG_ARCH_MEDIATEK) += mt8183-kukui-jacuzzi-willow-sku1.dtb
 dtb-$(CONFIG_ARCH_MEDIATEK) += mt8183-kukui-kakadu.dtb
diff --git a/arch/arm64/boot/dts/mediatek/mt8183-kukui-jacuzzi-makomo-sku0.dts b/arch/arm64/boot/dts/mediatek/mt8183-kukui-jacuzzi-makomo-sku0.dts
new file mode 100644
index 000000000000..51bf2893ec03
--- /dev/null
+++ b/arch/arm64/boot/dts/mediatek/mt8183-kukui-jacuzzi-makomo-sku0.dts
@@ -0,0 +1,24 @@
+// SPDX-License-Identifier: (GPL-2.0 OR MIT)
+/*
+ * Copyright 2021 Google LLC
+ */
+
+/dts-v1/;
+#include "mt8183-kukui-jacuzzi-fennel.dtsi"
+#include "mt8183-kukui-audio-da7219-rt1015p.dtsi"
+
+/ {
+	model = "Google makomo sku0 board";
+	compatible = "google,makomo-rev4-sku0", "google,makomo-rev5-sku0",
+		"google,makomo", "mediatek,mt8183";
+};
+
+&qca_wifi {
+	qcom,ath10k-calibration-variant = "GO_FENNEL14";
+};
+
+&mmc1_pins_uhs {
+	pins_clk {
+		drive-strength = <MTK_DRIVE_6mA>;
+	};
+};
diff --git a/arch/arm64/boot/dts/mediatek/mt8183-kukui-jacuzzi-makomo-sku1.dts b/arch/arm64/boot/dts/mediatek/mt8183-kukui-jacuzzi-makomo-sku1.dts
new file mode 100644
index 000000000000..c3b7e9bb0c89
--- /dev/null
+++ b/arch/arm64/boot/dts/mediatek/mt8183-kukui-jacuzzi-makomo-sku1.dts
@@ -0,0 +1,24 @@
+// SPDX-License-Identifier: (GPL-2.0 OR MIT)
+/*
+ * Copyright 2021 Google LLC
+ */
+
+/dts-v1/;
+#include "mt8183-kukui-jacuzzi-fennel.dtsi"
+#include "mt8183-kukui-audio-ts3a227e-rt1015p.dtsi"
+
+/ {
+	model = "Google makomo sku1 board";
+	compatible = "google,makomo-rev4-sku1", "google,makomo-rev5-sku1",
+		"google,makomo", "mediatek,mt8183";
+};
+
+&qca_wifi {
+	qcom,ath10k-calibration-variant = "GO_FENNEL14";
+};
+
+&mmc1_pins_uhs {
+	pins_clk {
+		drive-strength = <MTK_DRIVE_6mA>;
+	};
+};
-- 
2.39.1

