From 9172802977b738581bd9e3d8fd75fb6289ece97e Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Duje=20Mihanovi=C4=87?= <duje@dujemihanovic.xyz>
Date: Sat, 13 Sep 2025 23:21:11 +0200
Subject: [PATCH 12/21] arm64: dts: marvell: samsung,coreprimevelte: Add USB
 connector
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Add a node for the micro-USB connector found on the board.

Signed-off-by: Duje Mihanović <duje@dujemihanovic.xyz>
---
 .../boot/dts/marvell/mmp/pxa1908-samsung-coreprimevelte.dts | 6 ++++++
 1 file changed, 6 insertions(+)

diff --git a/arch/arm64/boot/dts/marvell/mmp/pxa1908-samsung-coreprimevelte.dts b/arch/arm64/boot/dts/marvell/mmp/pxa1908-samsung-coreprimevelte.dts
index 7fd5420937bd..10e6730d71b6 100644
--- a/arch/arm64/boot/dts/marvell/mmp/pxa1908-samsung-coreprimevelte.dts
+++ b/arch/arm64/boot/dts/marvell/mmp/pxa1908-samsung-coreprimevelte.dts
@@ -69,6 +69,12 @@ muic: extcon@14 {
 			reg = <0x14>;
 			interrupt-parent = <&gpio>;
 			interrupts = <0 IRQ_TYPE_EDGE_FALLING>;
+
+			usb_con: connector {
+				compatible = "usb-b-connector";
+				label = "micro-USB";
+				type = "micro";
+			};
 		};
 	};
 
-- 
2.52.0

